Table 11. summary of results
	Demand Capacity Ratios (%age) Linear Static Analysis Without Dynamic Increase Factor.
	DCR (%age) Linear Static Analysis as Per GSA 2016 Guidelines

	Critical Beam Elements
	Before Column Missing
	After Column Missing
	(Linear Static Analysis with DIF)
	Displacement at Column removed Joints

	
	Zone 2
	Zone 5
	Zone 2
	Zone 5
	
	

	
	Beam sections
	Beam sections
	
	

	B6B
	57%(230x230)
25%(530x300)
	70%(230x230)
49%(530x300)
	95%(230x230)
43%(530x300)
	56%(230x230)
34%(530x300)
	190%Max.
68%Min.
	
Case RC1
14.2mm (230X230) Maximum

3.96mm (530X300)  Minimum



Case RC2
13.1mm
(230X230) Maximum

3.6mm (530X300)  Minimum



Case RC3
13.4mm (230X230)
Maximum

4.26mm
(530X300)
Minimum

	B9B
	57%(230x230)
27%(530x300)
	74%(230x230)
49%(530x300)
	82%(230x230)
33%(530X300)
	49%(230x230)
24%(530X300)
	164%Max.
48%Min.
	

	B21B
	53%(230x230)
25%(530x300)
	62%(230x230)
47%(530x300)
	98%(230x230)
36%(530x300)
	53%(230x230)
30%(530x300)
	196%Max.
60% Min.
	

	B22B
	55%(230x230)
22%(530x300)
	61%(230x230)
46%(530x300)
	97%(230x230)
38%(530x300)
	52%(230x230)
31%(530X300)
	194% Max.
62% Min.
	

	B26B
	52%(230x230)
21%(530x300)
	62%(230x230)
46%(530x300)
	102%(230x230)
44%(530x300)
	57%(230x230)
37%(530x300)
	204% Max.
74% Min.
	

	Critical Column Elements
	

	C1
	37%(530x300)
8%(230x230)
	47%(300x230)
18%(230x230)’
	32%(530X300)  RC1
23%(230x230)  RC1
	25%(300X230) RC1
16%(530X230) RC1
	64% Max.
32% Min.
	

	C2
	24%(450x300)
7%(230x230)
	74%(380x230)
3%(300x230)
	1500%(450X300)RC1
59%(230X230) RC1
	46%(230x230) RC1
7%(530X300) RC1
	3000% Max.
14% Min.
	

	
	
	
	5200%(380X230)RC3
278%(230X230) RC3
	278%(230X230) RC3
24%(530X530)   RC3
	10400%
48% Min.
	

	C6
	58%(530x300)
10%(230x230)
	47%(300x230)
7%(530x300)
	3200%(530X300)RC1 90%(230X230) RC1
	115%(300X230) RC1 17%(530X230) RC1
	6400% Max.
 34% Min.
	

	
	
	
	1500%(530X300)RC2
75%(230X230) RC2
	107%(300X230) RC2
18%(530X300) RC2
	3000% Max.
36% Min.
	

	
	
	
	5%(530X300) RC3
1%(230X230) RC3
	2%(230X230) RC3
1%(530X300) RC3
	10% Max.
2% Min.
	

	C7
	41%(450x300)
11%(230x230)’
	59%(300x230)
26%(230x230)’
	1%(450x300) RC3
1%(230X230 )RC3
	1%(450X300) RC3
1%(300X230)
	2% Max.
2% Min.
	

	C8
	38%(450x300)
9%(230x230)
	74%(380x300)
20%(230x230)’
	1%(450x300) RC3
1%(ALL)
	2%(450X300) RC3
1%(230X230) RC3
	4% Max.
2% Min.
	

	C11
	62%(530x300)
12%(230x230)
	63%(300x230)
28%(230x230)’
	1%(ALL)RC2
	1%(ALL)RC2

	2% Max.
2% Min.
	

	C12
	52%(530x300)
9%(230x230)
	66%(380x300)
9%(380x230)
	1%(ALL)RC2 
	1%(ALL)RC2
	2% Max.
	

	
	
	
	FAIL IN FLEXURE(ALL) RC3
	FAIL INFLEXURE(ALL)RC3
	>200%
	

	C16
	58%(530x300)
10%(230x230)
	48%(300x230)
16%(530x300)
	1496%(450X300)RC2
75%(230X230) RC2
	107%(300X230) RC2
15%(530X300) RC2
	2992% Max.
30% Min.
	


Legend; DCR <100%-----No yielding.
100<DCR<200%----------Limited yielding.
DCR>200%----------------Large yielding.

