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Figure 1: 1H NMR spectrum of compound 4a (400 MHz, DMSO-d6)



Figure 2: 13C NMR spectrum of compound 4a (100.6 MHz, DMSO-d6)



Figure 3: 1H NMR spectrum of compound 4b (400 MHz, DMSO-d6)



Figure 4: 13C NMR spectrum of compound 4b (100.6 MHz, DMSO-d6)



Figure 5: 1H NMR spectrum of compound 4c (400 MHz, DMSO-d6)



Figure 6: 13C NMR spectrum of compound 4c (100.6 MHz, DMSO-d6)



Figure 7: 1H NMR spectrum of compound 4d (400 MHz, DMSO-d6)



Figure 8: 13C NMR spectrum of compound 4d (100.6 MHz, DMSO-d6)



Figure 9: 1H NMR spectrum of compound 4e (400 MHz, DMSO-d6)



Figure 10: 13C NMR spectrum of compound 4e (100.6 MHz, DMSO-d6)



Figure 11: 1H NMR spectrum of compound 4f (400 MHz, DMSO-d6)



Figure 12: 13C NMR spectrum of compound 4f (100.6 MHz, DMSO-d6)



Figure 13: 1H NMR spectrum of compound 4g (400 MHz, DMSO-d6)



Figure 14: 13C NMR spectrum of compound 4g (100.6 MHz, DMSO-d6)



Figure 15: 1H NMR spectrum of compound 4h (400 MHz, DMSO-d6)



Figure 16: 13C NMR spectrum of compound 4h (100.6 MHz, DMSO-d6)



Figure 17: 1H NMR spectrum of compound 4i (400 MHz, DMSO-d6)



Figure 18: 13C NMR spectrum of compound 4i (100.6 MHz, DMSO-d6)



Figure 19: 1H NMR spectrum of compound 4j (400 MHz, DMSO-d6)



Figure 20: 13C NMR spectrum of compound 4j (100.6 MHz, DMSO-d6)



Figure 21: 1H NMR spectrum of compound 4k (400 MHz, DMSO-d6)



Figure 22: 13C NMR spectrum of compound 4k (100.6 MHz, DMSO-d6)



Figure 23: 1H NMR spectrum of compound 4l (400 MHz, DMSO-d6)



Figure 24: 13C NMR spectrum of compound 4l (100.6 MHz, DMSO-d6)



Figure 25: 1H NMR spectrum of compound 4m (400 MHz, DMSO-d6)



Figure 26: 13C NMR spectrum of compound 4m (100.6 MHz, DMSO-d6)



Figure 27: 1H NMR spectrum of compound 4n (400 MHz, DMSO-d6)



Figure 28: 13C NMR spectrum of compound 4n (100.6 MHz, DMSO-d6)
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