Nco match to nca asgn search completed.
The protein amino acid sequence is:
The protein sequence read from  RSV_seq.txt  is: 
PVVIKTEGPA   WTPLEPKLIT   RLADTVRTKG   LRSPITMAEV   EALMSSPLLP
HDVTNLMRVI   LGPAPYALWM   DAWGVQLQTV   IAAATRDPRH   PANGQGRGER
TNLNRLKGLA   DGMVGNPQGQ   AALLRPGELV   AITASALQAF   REVARLAEPA
GPWADIMQGP   SESFVDFANR   LIKAVEGSDL   PPSARAPVII   DCFRQKSQPD
IQQLIRTAPS   TLTTPGEIIK   YVLDRQKTAP   

The following is the breakdown of sequence composition and residue types in the input nca asignments.
amino acid types             num of copies in sequence         num of copies in ncacx input        num of definitely asgned in ncacx input        num of copies free from local minimum concerns in ncacx input
A            28              28          15          18
C            1              1          0          1
D            11              11          7          11
E            11              11          3          11
F            4              4          3          4
G            16              16          11          16
H            2              2          0          2
I            14              14          11          10
K            8              8          7          8
L            24              24          15          22
M            6              6          5          4
N            6              6          4          5
P            23              23          7          13
Q            12              12          6          11
R            17              17          8          16
S            10              10          9          10
T            16              16          12          14
V            15              15          6          12
W            4              4          2          4
Y            2              2          2          2


Input statistics:
There are  133  sequentially assigned nca asgn pre-existing in ncacx input
There are additional  97  none definite nca asgn.
There are  414  individual resonances(peaks) from ncocx input.
There are  19 individual nco resonances(peaks) not used for match finding.


Matching results:
There are  26  nca inputs do not have matched nco
There are  167 nca inputs have 1 unique matched nco
There are  14  nca inputs have 2 matched nco
There are  7  nca inputs have 3 matched nco
There are  4  nca inputs have 4 matched nco
There are  2  nca inputs have 5 matched nco
There are  145  nca inputs have non-overlaping and unique nco match.
There are additional  6  nca inputs have non-overlaping and non unique nco match.


Overlaping definition: if any nco signals used in a match is used more than 
its specified degeneracy values in the entire nco to nca match search process.
################################################################
There are  26 ncacx inputs with no nco matches, and they are:
ncacx row  1 1000000.0 1000000.0  1000000.0  1000000.0  1 P
ncacx row  6 116.5 1000000.0  59.21  65.96  1 T
ncacx row  7 125.7 1000000.0  54.9  32.16  1 E
ncacx row  9 134.8 1000000.0  64.3  31.72  1 P
ncacx row  11 1000000.0 1000000.0  1000000.0  1000000.0  1 W
ncacx row  15 123.6 1000000.0  54.29  30.2  1 E
ncacx row  17 116.5 1000000.0  59.7  32.29  1 K
ncacx row  46 118.8 1000000.0  56.0  64.21  1 S
ncacx row  47 140.4 176.2  64.58  32.29  1 P
ncacx row  87 116.6 1000000.0  49.57  42.67  1 D
ncacx row  90 124.4 172.8  57.1  32.17  1 H
ncacx row  116 112.4 172.1  49.8  38.5  1 N
ncacx row  125 123.1 176.6  54.43  30.32  1 R
ncacx row  145 113.3 179.3  58.5  30.46  1 R
ncacx row  146 119.2 177.1  56.4  43.34  1 L
ncacx row  150 1000000.0 1000000.0  1000000.0  1000000.0  1 A
ncacx row  153 119.3 1000000.0  62.9  28.6  1 W
ncacx row  158 126.7 178.8  56.2  27.81  1 Q
ncacx row  164 124.5 177.1  63.13  39.3  1 F
ncacx row  180 122.4 1000000.0  54.92  42.92  1 L
ncacx row  192 118.5 1000000.0  56.76  27.2  1 C
ncacx row  208 125.0 1000000.0  50.4  22.44  1 A
ncacx row  222 118.8 1000000.0  66.03  29.95  1 V
ncacx row  224 119.6 1000000.0  56.88  40.62  1 D
ncacx row  226 118.5 1000000.0  59.2  29.4  1 Q
ncacx row  229 1000000.0 1000000.0  1000000.0  1000000.0  1 A
################################################################
We find  167  ncacx inputs have a unique matched nco residue type assignments:
ncacx row  2 121.9 175.3  61.81  34.98  1 V
its nco match is 
125.4 175.1  61.9  34.7

ncacx row  3 125.4 174.0  59.56  35.01  1 V3
its nco match is 
125.4 173.8  59.5  35.0

ncacx row  4 125.4 175.9  60.99  36.2  1 I4
its nco match is 
128.6 175.7  61.0  36.3

ncacx row  5 128.6 178.5  54.97  34.18  1 K5
its nco match is 
116.7 178.5  54.86  33.91

ncacx row  10 123.1 1000000.0  52.05  20.1  1 A
its nco match is 
120.7 176.1  52.0  19.7

ncacx row  12 124.7 170.2  57.26  71.06  1 T12
its nco match is 
137.8 170.1  57.1  71.0

ncacx row  13 138.0 176.7  61.7  1000000.0  1 P13
its nco match is 
122.7 176.7  62.0

ncacx row  14 122.8 1000000.0  54.9  43.0  1 L14
its nco match is 
123.7 176.9  55.1  42.97

ncacx row  19 119.8 178.6  64.61  37.84  1 I19
its nco match is 
117.7 178.6  64.9  37.63

ncacx row  20 117.6 176.2  66.7  68.6  1 T20
its nco match is 
121.2 176.1  68.3  67.09

ncacx row  21 121.4 178.5  59.6  30.07  1 R
its nco match is 
121.3 178.6  59.3  30.0

ncacx row  23 122.2 180.9  54.95  17.82  1 A23
its nco match is 
119.5 180.9  54.83  17.9

ncacx row  24 119.6 1000000.0  57.3  40.62  1 D71
its nco match is 
122.3 178.7  57.56  40.82

ncacx row  25 122.1 1000000.0  67.21  68.24  1 T25
its nco match is 
121.6 176.1  67.07  68.27

ncacx row  27 118.7 177.9  59.56  30.74  1 R27
its nco match is 
107.9 177.9  59.63  30.94

ncacx row  28 107.8 176.6  63.88  70.4  1 T28
its nco match is 
119.8 176.4  63.9  70.4

ncacx row  29 120.0 1000000.0  55.71  32.59  1 K29
its nco match is 
107.7 178.0  55.61  32.5

ncacx row  30 107.7 173.8  44.46  1000000.0  1 G
its nco match is 
117.9 173.8  44.8

ncacx row  31 120.3 1000000.0  55.63  43.0  1 L31
its nco match is 
113.1 176.0  55.69  43.3  55.72  42.91

ncacx row  32 112.8 176.6  55.46  31.13  1 R
its nco match is 
113.8 176.5  55.4  31.3

ncacx row  33 113.9 1000000.0  55.25  64.42  1 S33
its nco match is 
140.3 173.9  55.32  64.36  55.35  64.4

ncacx row  35 119.1 1000000.0  60.5  38.1  1 I172
its nco match is 
118.5 176.6  60.2  38.4

ncacx row  36 118.6 1000000.0  66.46  68.64  1 T79
its nco match is 
125.2 177.1  66.4  68.6

ncacx row  37 118.3 1000000.0  57.84  32.47  1 M37
its nco match is 
120.3 177.6  57.74  32.25

ncacx row  40 120.5 1000000.0  67.25  32.14  1 V165
its nco match is 
121.3 176.1  67.09  31.8

ncacx row  41 119.0 179.2  60.5  30.07  1 E
its nco match is 
119.8 179.2  60.47  29.99

ncacx row  43 120.2 178.0  58.26  42.1  1 L43
its nco match is 
114.2 177.9  58.33  42.26

ncacx row  44 114.3 174.7  55.68  33.64  1 M44
its nco match is 
112.6 174.7  55.55  33.8

ncacx row  45 112.5 1000000.0  60.43  63.71  1 S45
its nco match is 
118.9 174.9  60.4  63.7

ncacx row  48 125.0 174.4  53.85  45.0  1 L48
its nco match is 
112.8 174.3  53.93  44.62

ncacx row  49 112.5 174.9  52.38  41.2  1 L49
its nco match is 
137.2 174.9  52.38  41.47

ncacx row  51 116.2 1000000.0  60.34  31.29  1 H
its nco match is 
114.2 177.4  60.52  31.4

ncacx row  52 115.9 1000000.0  57.2  39.4  1 D52
its nco match is 
115.4 178.2  57.4  39.8

ncacx row  53 115.6 1000000.0  66.07  31.93  1 V53
its nco match is 
112.2 176.7  65.88  32.14

ncacx row  54 111.9 176.9  65.83  68.15  1 T54
its nco match is 
118.3 176.7  66.01  68.3

ncacx row  55 118.6 176.1  57.4  38.76  1 N55
its nco match is 
120.2 175.9  57.7  38.74

ncacx row  56 120.2 1000000.0  58.3  42.4  1 L56
its nco match is 
114.6 177.9  58.36  42.15

ncacx row  57 114.7 1000000.0  56.4  30.56  1 M57
its nco match is 
118.5 177.3  56.6  30.88

ncacx row  59 115.4 1000000.0  65.57  31.83  1 V59
its nco match is 
109.2 177.7  65.52  32.05

ncacx row  60 109.2 175.1  63.53  39.07  1 I60
its nco match is 
118.8 174.8  63.62  38.9

ncacx row  61 118.7 1000000.0  52.98  44.17  1 L61
its nco match is 
103.2 177.1  53.2  43.96

ncacx row  64 119.2 176.0  57.09  15.49  1 A186
its nco match is 
131.9 176.0  15.44  56.99

ncacx row  65 131.7 1000000.0  65.84  31.7  1 P
its nco match is 
119.1 177.2  65.97  31.5

ncacx row  66 118.8 1000000.0  62.46  38.25  1 Y66
its nco match is 
122.7 176.7  62.3  38.2

ncacx row  68 118.3 1000000.0  56.4  43.34  1 L68
its nco match is 
121.5 176.3  56.6  43.5

ncacx row  69 121.2 1000000.0  57.0  28.4  1 W69
its nco match is 
120.8 177.1  57.11  28.12

ncacx row  70 121.0 1000000.0  57.93  31.23  1 M70
its nco match is 
119.2 179.3  58.3  31.23

ncacx row  71 119.9 1000000.0  57.1  40.7  1 D24
its nco match is 
122.3 178.5  57.4  40.8

ncacx row  73 123.3 1000000.0  59.7  26.97  1 W73
its nco match is 
103.5 177.5  59.95  26.96

ncacx row  74 103.8 176.2  47.73  1000000.0  1 G74
its nco match is 
122.1 176.1  47.71

ncacx row  76 119.0 1000000.0  60.5  29.14  1 Q
its nco match is 
120.0 179.5  60.47  29.34

ncacx row  77 120.2 1000000.0  58.29  42.4  1 L
its nco match is 
118.3 179.7  58.25  42.68

ncacx row  78 118.5 1000000.0  59.14  28.01  1 Q
its nco match is 
116.9 179.1  59.24  28.07

ncacx row  79 117.1 177.1  66.48  68.69  1 T211
its nco match is 
124.7 177.0  66.3  68.3

ncacx row  80 125.4 177.4  66.06  31.03  1 V80
its nco match is 
118.7 177.3  66.1  30.9

ncacx row  81 118.5 1000000.0  63.2  35.95  1 I81
its nco match is 
124.5 178.9  63.24  36.05

ncacx row  82 124.2 1000000.0  54.95  17.86  1 A82
its nco match is 
120.0 180.9  54.84  17.9  55.0  17.78

ncacx row  84 120.8 1000000.0  53.16  17.42  1 A84
its nco match is 
113.9 178.8  53.38  17.46

ncacx row  85 113.8 174.8  65.35  69.1  1 T85
its nco match is 
119.5 175.0  65.4  69.1

ncacx row  86 119.4 175.7  57.54  31.08  1 R86
its nco match is 
116.5 175.8  57.5  31.1

ncacx row  88 139.4 178.1  64.5  32.9  1 P
its nco match is 
115.3 178.1  64.4  32.9

ncacx row  89 115.1 175.7  55.64  29.44  1 R89
its nco match is 
124.6 175.6  55.63  29.36

ncacx row  93 117.1 1000000.0  54.54  41.07  1 N
its nco match is 
121.2 176.6  54.6  41.2

ncacx row  94 107.7 173.8  44.5  1000000.0  1 G30
its nco match is 
120.0 173.9  44.4

ncacx row  95 118.3 177.8  56.5  29.66  1 Q95
its nco match is 
108.6 177.8  56.37  29.78

ncacx row  96 108.6 173.8  44.1  1000000.0  1 G96
its nco match is 
119.9 173.8  44.3

ncacx row  97 119.6 176.7  57.54  31.08  1 R
its nco match is 
112.4 176.5  57.63  31.12

ncacx row  98 112.1 174.7  45.0  1000000.0  1 G98
its nco match is 
121.7 174.7  44.7

ncacx row  99 121.6 1000000.0  57.01  28.4  1 E
its nco match is 
121.3 177.3  57.11  28.07

ncacx row  100 121.3 178.5  55.34  31.49  1 R100
its nco match is 
117.7 178.6  55.44  31.3

ncacx row  101 117.7 172.8  63.34  66.36  1 T
its nco match is 
113.6 172.8  63.0  66.3

ncacx row  102 113.3 174.3  53.5  40.2  1 N102
its nco match is 
120.2 174.2  53.2  40.2

ncacx row  103 120.2 177.2  58.3  42.4  1 L103
its nco match is 
115.0 177.1  58.3  42.4

ncacx row  104 115.0 178.5  56.1  37.0  1 N169
its nco match is 
120.7 178.5  56.1  37.0

ncacx row  105 120.6 177.8  60.7  31.1  1 R170
its nco match is 
122.2 178.0  60.78  31.4

ncacx row  106 113.3 175.2  57.1  41.4  1 L106
its nco match is 
108.0 175.1  57.1  41.5

ncacx row  107 107.7 177.8  56.4  34.4  1 K107
its nco match is 
108.3 177.8  56.4  34.4

ncacx row  108 108.6 174.0  46.9  1000000.0  1 G108
its nco match is 
115.8 173.9  46.7

ncacx row  109 115.7 176.4  53.9  43.6  1 L109
its nco match is 
121.5 176.3  43.55  53.9

ncacx row  110 121.4 175.9  50.9  19.6  1 A110
its nco match is 
120.1 176.1  50.6  19.6

ncacx row  111 119.9 176.8  57.0  40.7  1 D111
its nco match is 
112.1 176.9  56.8  40.7

ncacx row  112 112.0 174.6  45.1  1000000.0  1 G112
its nco match is 
113.0 174.6  44.9

ncacx row  113 113.3 177.4  57.3  34.6  1 M113
its nco match is 
121.6 177.2  57.1  34.6

ncacx row  114 121.4 178.6  64.9  31.0  1 V
its nco match is 
118.4 178.6  64.9  30.9

ncacx row  115 118.1 174.7  46.5  1000000.0  1 G115
its nco match is 
112.2 174.6  46.39

ncacx row  118 115.5 179.2  59.71  26.96  1 Q118
its nco match is 
109.3 179.1  60.13  26.95

ncacx row  119 109.2 176.0  46.89  1000000.0  1 G119
its nco match is 
119.7 175.9  47.1

ncacx row  121 118.9 180.2  54.79  18.5  1 A121
its nco match is 
117.1 180.0  54.6  18.38

ncacx row  122 117.1 180.0  54.0  18.9  1 A122
its nco match is 
115.3 180.0  53.9  19.1

ncacx row  123 115.3 179.1  56.59  45.8  1 L123
its nco match is 
120.2 179.1  56.6  45.72

ncacx row  124 120.3 1000000.0  55.63  42.77  1 L
its nco match is 
123.3 176.9  55.66  42.91

ncacx row  126 137.8 179.4  66.72  32.12  1 P126
its nco match is 
101.9 179.5  66.62  32.03

ncacx row  127 102.3 178.4  46.65  1000000.0  1 G127
its nco match is 
119.7 178.6  46.59

ncacx row  128 119.4 176.2  60.3  29.13  1 E128
its nco match is 
117.8 176.2  60.52  29.14

ncacx row  129 117.9 180.8  58.2  41.33  1 L129
its nco match is 
120.5 180.8  58.5  41.4

ncacx row  131 122.6 181.6  54.99  19.04  1 A
its nco match is 
123.3 181.8  54.92  18.99

ncacx row  132 123.1 177.9  66.83  39.8  1 I132
its nco match is 
117.6 178.0  66.85  39.66

ncacx row  133 117.6 1000000.0  66.61  68.5  1 T
its nco match is 
124.7 177.1  66.3  68.46

ncacx row  134 124.8 182.2  55.5  18.26  1 A134
its nco match is 
113.5 182.2  55.54  18.23

ncacx row  135 113.2 176.2  62.61  63.48  1 S135
its nco match is 
125.9 176.2  62.8  63.3

ncacx row  136 126.0 1000000.0  56.26  20.56  1 A136
its nco match is 
122.3 180.5  56.32  20.58

ncacx row  138 119.5 1000000.0  58.3  28.36  1 Q138
its nco match is 
126.4 176.1  58.33  28.2

ncacx row  139 126.4 1000000.0  55.3  20.6  1 A139
its nco match is 
119.0 177.3  55.45  20.8

ncacx row  140 119.0 1000000.0  62.98  38.88  1 F140
its nco match is 
118.9 176.1  39.0  63.15

ncacx row  141 119.0 177.2  60.58  29.86  1 R141
its nco match is 
117.3 177.2  60.56  30.1

ncacx row  142 117.5 176.3  59.5  28.1  1 E142
its nco match is 
121.9 176.3  59.6  28.3

ncacx row  144 123.0 177.1  55.1  17.12  1 A144
its nco match is 
113.2 177.1  54.9  17.4

ncacx row  148 137.5 1000000.0  50.1  28.01  1 E
its nco match is 
136.6 177.7  49.8  28.0

ncacx row  149 136.6 1000000.0  61.23  1000000.0  1 P
its nco match is 
119.1 176.3  61.2

ncacx row  151 107.7 174.0  44.45  1000000.0  1 G
its nco match is 
117.9 173.8  44.8

ncacx row  154 123.0 1000000.0  55.2  17.1  1 A
its nco match is 
117.0 181.5  55.3  17.1

ncacx row  155 117.1 1000000.0  54.5  41.1  1 D179
its nco match is 
122.4 177.9  54.8  40.8

ncacx row  156 120.9 1000000.0  66.3  38.1  1 I189
its nco match is 
117.2 176.3  66.43  37.9

ncacx row  157 118.7 1000000.0  60.51  30.02  1 M
its nco match is 
119.8 179.2  60.47  29.99

ncacx row  160 135.0 177.8  65.13  31.69  1 P160
its nco match is 
112.5 177.8  64.93  31.67

ncacx row  161 112.6 173.1  56.81  63.7  1 S161
its nco match is 
125.8 173.0  56.9  63.75

ncacx row  162 125.7 176.7  54.93  32.19  1 E162
its nco match is 
127.6 176.5  54.94  32.21

ncacx row  163 127.4 175.1  58.36  64.23  1 S163
its nco match is 
124.2 175.1  58.31  64.16

ncacx row  165 116.5 176.1  67.09  31.81  1 V
its nco match is 
121.2 176.1  67.0  31.8

ncacx row  166 121.3 179.3  58.26  39.96  1 D166
its nco match is 
123.3 179.1  58.26  39.91

ncacx row  167 123.3 175.4  59.21  39.06  1 F167
its nco match is 
121.9 175.5  59.31  38.98

ncacx row  168 122.0 177.8  54.58  18.2  1 A168
its nco match is 
115.3 177.8  54.61  18.5

ncacx row  169 115.2 179.3  56.56  38.09  1 N104
its nco match is 
120.6 179.3  56.5  37.8

ncacx row  170 120.6 177.8  60.73  31.1  1 R105
its nco match is 
113.2 177.5  60.7  31.2

ncacx row  173 118.7 1000000.0  60.18  32.76  1 K173
its nco match is 
120.9 179.5  60.0  60.0  32.95  60.0

ncacx row  174 120.9 1000000.0  54.9  18.5  1 A174
its nco match is 
117.5 177.2  54.5  18.5

ncacx row  175 117.6 1000000.0  67.23  31.7  1 V188
its nco match is 
120.9 180.3  67.32  31.63

ncacx row  177 103.0 174.0  44.96  1000000.0  1 G177
its nco match is 
117.9 173.8  44.94

ncacx row  178 117.7 173.4  58.93  65.83  1 S178
its nco match is 
116.9 173.4  59.1  65.8

ncacx row  179 117.0 1000000.0  54.55  41.04  1 D
its nco match is 
121.2 176.6  54.6  41.2

ncacx row  181 138.0 175.9  61.64  1000000.0  1 P181
its nco match is 
135.9 175.9  61.3

ncacx row  182 136.2 1000000.0  66.8  32.41  1 P182
its nco match is 
110.2 179.1  66.4  32.27

ncacx row  183 110.3 174.8  60.48  62.62  1 S183
its nco match is 
122.2 174.7  60.41  62.59

ncacx row  184 122.2 1000000.0  51.9  20.01  1 A184
its nco match is 
115.7 177.7  52.09  20.07

ncacx row  185 115.8 176.4  61.0  30.35  1 R
its nco match is 
119.1 176.3  61.2  30.41

ncacx row  186 119.2 1000000.0  57.09  15.49  1 A64
its nco match is 
131.9 176.0  56.99  15.44

ncacx row  187 131.7 179.3  66.03  1000000.0  1 P187
its nco match is 
117.5 179.3  65.96

ncacx row  188 117.6 176.2  67.23  31.72  1 V
its nco match is 
121.2 176.1  67.0  31.8

ncacx row  190 117.2 1000000.0  66.6  37.77  1 I190
its nco match is 
120.9 180.2  66.8  37.5

ncacx row  191 121.2 1000000.0  58.08  40.2  1 D191
its nco match is 
118.5 179.8  58.2  40.4

ncacx row  193 118.5 1000000.0  62.0  39.5  1 F193
its nco match is 
116.4 177.7  61.9  39.4

ncacx row  194 116.3 178.1  60.05  31.71  1 R194
its nco match is 
113.2 177.8  60.3  31.66

ncacx row  195 113.0 1000000.0  57.34  32.14  1 Q195
its nco match is 
114.9 177.9  57.1  32.3

ncacx row  196 115.1 1000000.0  55.64  29.44  1 K196
its nco match is 
113.1 177.4  55.63  29.51

ncacx row  197 113.1 1000000.0  57.29  65.05  1 S197
its nco match is 
121.0 177.2  57.05  64.95

ncacx row  198 121.0 1000000.0  55.75  28.4  1 Q198
its nco match is 
136.9 175.5  55.82  28.1

ncacx row  200 115.9 178.6  57.15  39.33  1 D
its nco match is 
123.4 178.6  57.4  39.31

ncacx row  201 123.4 178.3  62.57  36.27  1 I201
its nco match is 
119.5 178.4  62.47  36.16

ncacx row  202 119.7 1000000.0  60.3  28.9  1 Q202
its nco match is 
126.7 173.7  60.7  29.17  60.6  28.79

ncacx row  203 115.7 1000000.0  60.97  27.89  1 Q
its nco match is 
120.7 178.5  60.6  27.7

ncacx row  204 120.9 1000000.0  58.04  42.39  1 L204
its nco match is 
118.8 179.3  58.2  42.7

ncacx row  206 119.8 1000000.0  60.45  31.18  1 R
its nco match is 
114.2 177.4  60.52  31.4

ncacx row  207 118.9 1000000.0  66.2  68.1  1 T36
its nco match is 
118.3 176.7  66.0  68.1

ncacx row  209 135.5 1000000.0  62.97  1000000.0  1 P209
its nco match is 
117.4 177.3  63.0

ncacx row  210 117.4 173.4  58.9  65.8  1 S210
its nco match is 
117.2 173.5  59.16  65.95

ncacx row  211 117.2 175.5  68.1  69.0  1 T133
its nco match is 
124.7 175.5  68.21  69.2

ncacx row  212 124.5 1000000.0  53.7  44.7  1 L212
its nco match is 
111.7 174.4  53.5  44.9

ncacx row  213 111.8 174.5  62.9  71.0  1 T213
its nco match is 
110.1 174.2  62.69  70.9

ncacx row  214 110.3 173.3  58.14  69.82  1 T214
its nco match is 
131.8 173.2  58.5  69.8

ncacx row  216 103.1 175.9  47.4  1000000.0  1 G216
its nco match is 
119.5 175.8  47.08

ncacx row  218 121.1 1000000.0  62.56  37.09  1 I218
its nco match is 
120.4 178.2  62.47  37.03

ncacx row  219 120.3 1000000.0  66.49  38.07  1 I219
its nco match is 
117.3 176.8  66.4  37.9

ncacx row  220 117.3 1000000.0  59.7  33.0  1 K220
its nco match is 
119.2 179.0  59.4  32.7

ncacx row  221 119.0 1000000.0  62.98  38.88  1 Y221
its nco match is 
118.9 176.1  63.2  39.06

ncacx row  227 119.6 1000000.0  57.78  31.18  1 K17
its nco match is 
119.8 179.3  60.0  31.94  58.2  31.4

ncacx row  228 114.4 174.1  55.5  64.66  1 T
its nco match is 
140.2 173.9  55.5  64.36

ncacx row  230 140.6 1000000.0  64.6  32.3  1 P
its nco match is 
119.2 178.8  64.86  32.0

################################################################
We find  14  ncacx inputs have 2 matched nco residue type assignments:
ncacx row  34 140.6 178.8  64.58  32.29  1 P
its first nco match is 
119.2 178.8  64.86  32.0

its 2nd nco match is 
119.2 179.2  64.8  32.0

ncacx row  39 119.8 1000000.0  60.2  28.9  1 E
its first nco match is 
118.6 177.2  59.94  28.76

its 2nd nco match is 
103.1 177.5  59.95  29.06

ncacx row  42 120.0 180.9  55.08  18.1  1 A
its first nco match is 
119.8 180.9  54.83  17.8

its 2nd nco match is 
121.1 180.5  54.86  18.37

ncacx row  58 118.5 1000000.0  59.2  28.2  1 R
its first nco match is 
115.7 178.9  59.35  28.5

its 2nd nco match is 
116.9 179.1  59.24  28.07

ncacx row  67 122.7 1000000.0  54.86  18.43  1 A
its first nco match is 
118.0 177.7  54.92  18.24

its 2nd nco match is 
121.1 180.5  54.86  18.37

ncacx row  83 122.7 1000000.0  54.86  18.43  1 A
its first nco match is 
118.0 177.7  54.92  18.24

its 2nd nco match is 
121.1 180.5  54.86  18.37

ncacx row  92 122.6 1000000.0  54.99  19.04  1 A
its first nco match is 
117.1 177.8  54.92  19.04

its 2nd nco match is 
123.3 181.8  54.92  18.99

ncacx row  117 139.4 177.5  64.5  1000000.0  1 P
its first nco match is 
122.8 177.1  64.5

its 2nd nco match is 
115.7 177.5  64.42

ncacx row  120 119.8 177.2  60.2  28.9  1 Q
its first nco match is 
118.6 177.2  59.94  28.76

its 2nd nco match is 
103.1 177.5  59.95  29.06

ncacx row  147 123.1 1000000.0  52.02  20.0  1 A
its first nco match is 
120.1 174.9  51.9  19.62

its 2nd nco match is 
120.7 176.1  52.0  19.7

ncacx row  159 119.5 173.4  44.95  1000000.0  1 G
its first nco match is 
117.9 173.8  44.8

its 2nd nco match is 
134.7 173.3  44.88

ncacx row  176 120.8 177.6  60.08  29.09  1 E
its first nco match is 
118.6 177.2  59.94  28.76

its 2nd nco match is 
103.1 177.5  59.95  29.06

ncacx row  217 120.1 1000000.0  60.2  28.9  1 E
its first nco match is 
118.6 177.2  59.94  28.76

its 2nd nco match is 
103.1 177.5  59.95  29.06

ncacx row  225 118.4 1000000.0  56.4  29.74  1 R
its first nco match is 
119.8 178.8  56.5  29.46

its 2nd nco match is 
118.2 178.4  56.28  29.7

################################################################
We find  7  ncacx inputs have 3 matched nco residue type assignments:
ncacx row  8 107.7 171.5  44.3  1000000.0  1 G
its first nco match is 
134.5 171.3  44.16

its 2nd nco match is 
134.8 171.3  44.12

its 3rd nco match is 
134.5 171.4  44.16

ncacx row  18 119.6 1000000.0  57.4  41.62  1 L
its first nco match is 
119.9 178.5  57.7  41.7

its 2nd nco match is 
119.9 178.5  57.7  41.7

its 3rd nco match is 
122.2 178.6  57.79  41.8

ncacx row  62 103.2 171.4  44.35  1000000.0  1 G
its first nco match is 
134.5 171.3  44.16

its 2nd nco match is 
134.8 171.3  44.12

its 3rd nco match is 
134.5 171.4  44.16

ncacx row  63 134.8 179.2  65.0  1000000.0  1 P
its first nco match is 
119.2 178.8  64.86

its 2nd nco match is 
119.2 179.2  64.8

its 3rd nco match is 
119.5 179.2  64.8

ncacx row  130 120.5 178.12  67.25  32.14  1 V
its first nco match is 
122.5 178.1  67.24  32.07

its 2nd nco match is 
123.0 178.0  67.2  32.12

its 3rd nco match is 
115.7 178.2  66.85  32.28

ncacx row  143 121.8 178.0  66.9  31.9  1 V
its first nco match is 
122.5 178.1  67.24  32.07

its 2nd nco match is 
123.0 178.0  67.2  32.12

its 3rd nco match is 
115.7 178.2  66.85  32.28

ncacx row  205 119.0 1000000.0  66.08  38.43  1 I
its first nco match is 
119.0 177.1  66.1  38.1

its 2nd nco match is 
119.1 177.1  66.04  38.13

its 3rd nco match is 
119.5 177.2  65.97  38.13

################################################################
We find  4  ncacx inputs have 4 matched nco residue type assignments:
ncacx row  38 120.1 1000000.0  55.01  18.22  1 A
its first nco match is 
119.8 180.9  54.83  17.8

its 2nd nco match is 
118.0 177.7  54.92  18.24

its 3rd nco match is 
123.3 178.4  54.7  18.0

its 4th nco match is 
121.1 180.5  54.86  18.37

ncacx row  72 122.3 1000000.0  54.51  18.2  1 A
its first nco match is 
119.8 180.9  54.83  17.8

its 2nd nco match is 
118.0 177.7  54.92  18.24

its 3rd nco match is 
123.3 178.4  54.7  18.0

its 4th nco match is 
121.1 180.5  54.86  18.37

ncacx row  172 119.0 176.8  66.09  38.4  1 I
its first nco match is 
119.1 177.2  65.97  38.13

its 2nd nco match is 
119.0 177.1  66.1  38.1

its 3rd nco match is 
119.1 177.1  66.04  38.13

its 4th nco match is 
119.5 177.2  65.97  38.13

ncacx row  189 120.8 176.9  66.29  38.1  1 I
its first nco match is 
119.1 177.2  65.97  38.13

its 2nd nco match is 
119.0 177.1  66.1  38.1

its 3rd nco match is 
119.1 177.1  66.04  38.13

its 4th nco match is 
119.5 177.2  65.97  38.13

################################################################
We find  2  ncacx inputs have five matched nco residue type assignments:
ncacx row  137 122.2 178.4  58.14  41.7  1 L
its first nco match is 
122.2 178.6  57.79  41.8

its 2nd nco match is 
119.5 178.4  58.1  41.7

its 3rd nco match is 
119.3 178.3  58.07  41.7

its 4th nco match is 
119.9 178.5  58.04  41.7

its 5th nco match is 
119.9 178.5  58.04  41.7

ncacx row  171 122.2 1000000.0  58.14  41.7  1 L
its first nco match is 
122.2 178.6  57.79  41.8

its 2nd nco match is 
119.5 178.4  58.1  41.7

its 3rd nco match is 
119.3 178.3  58.07  41.7

its 4th nco match is 
119.9 178.5  58.04  41.7

its 5th nco match is 
119.9 178.5  58.04  41.7

################################################################
The following list the nco signals never used in match finding:
nco signal index  1  from row number  1  in the original ncocx input file is not used.
Its coordn are  121.8 171.3 62.4 T
nco signal index  2  from row number  2  in the original ncocx input file is not used.
Its coordn are  121.8 171.3 32.2 I
nco signal index  18  from row number  18  in the original ncocx input file is not used.
Its coordn are  124.4 168.2 27.9 W
nco signal index  24  from row number  24  in the original ncocx input file is not used.
Its coordn are  139.1 176.2 54.97 E
nco signal index  25  from row number  25  in the original ncocx input file is not used.
Its coordn are  139.1 176.2 30.4 E
nco signal index  86  from row number  86  in the original ncocx input file is not used.
Its coordn are  125.2 176.2 32.78 P
nco signal index  91  from row number  91  in the original ncocx input file is not used.
Its coordn are  116.0 178.2 66.85 P
nco signal index  115  from row number  115  in the original ncocx input file is not used.
Its coordn are  119.2 179.2 31.41 P
nco signal index  160  from row number  160  in the original ncocx input file is not used.
Its coordn are  139.5 171.9 49.57 D
nco signal index  165  from row number  165  in the original ncocx input file is not used.
Its coordn are  131.6 172.8 56.8 H
nco signal index  208  from row number  208  in the original ncocx input file is not used.
Its coordn are  139.5 172.3 50.29 N
nco signal index  223  from row number  223  in the original ncocx input file is not used.
Its coordn are  137.9 176.7 54.59 R
nco signal index  273  from row number  273  in the original ncocx input file is not used.
Its coordn are  119.5 179.2 31.4 P
nco signal index  295  from row number  295  in the original ncocx input file is not used.
Its coordn are  116.8 177.1 39.42 F
nco signal index  327  from row number  327  in the original ncocx input file is not used.
Its coordn are  135.9 175.9 30.75 P
nco signal index  405  from row number  405  in the original ncocx input file is not used.
Its coordn are  118.4 179.5 40.56 D
nco signal index  408  from row number  408  in the original ncocx input file is not used.
Its coordn are  119.3 178.9 59.3 Q
nco signal index  409  from row number  409  in the original ncocx input file is not used.
Its coordn are  114.4 176.1 57.76 K227
nco signal index  410  from row number  410  in the original ncocx input file is not used.
Its coordn are  114.4 176.1 31.21 K227
################################################################
The following list the nco signals used more than their given degeneracy values (overused) in match finding:
nco signal index  13  from row number  13  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  134.5 171.3 44.16 G
nco signal index  14  from row number  14  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  122.8 177.1 64.5 P
nco signal index  26  from row number  26  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.7 176.8 64.51 P1
nco signal index  29  from row number  29  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  119.9 178.5 57.7 L
nco signal index  30  from row number  30  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  119.9 178.5 41.7 L
nco signal index  33  from row number  33  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  121.2 176.1 67.0 V
nco signal index  37  from row number  37  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  122.2 178.6 57.79 L
nco signal index  38  from row number  38  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  122.2 178.6 41.8 L
nco signal index  45  from row number  45  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  118.9 179.3 66.83 V
nco signal index  46  from row number  46  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  12  times in match finding.
Its coordn are  118.9 179.3 31.77 V
nco signal index  60  from row number  60  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.2 178.8 64.86 P
nco signal index  61  from row number  61  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.2 178.8 32.0 P
nco signal index  68  from row number  68  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.8 180.9 54.83 A
nco signal index  69  from row number  69  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.8 180.9 17.8 A
nco signal index  71  from row number  71  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  118.9 179.3 66.82 V
nco signal index  72  from row number  72  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  12  times in match finding.
Its coordn are  118.9 179.3 31.94 V
nco signal index  73  from row number  73  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.8 179.2 60.47 E
nco signal index  74  from row number  74  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.8 179.2 29.99 E
nco signal index  84  from row number  84  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  140.2 173.9 64.36 T207
nco signal index  85  from row number  85  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  125.2 176.2 64.58 P47
nco signal index  113  from row number  113  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  134.8 171.3 44.12 G
nco signal index  114  from row number  114  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.2 179.2 64.8 P
nco signal index  118  from row number  118  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.1 177.2 65.97 P
nco signal index  122  from row number  122  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.0 177.7 54.92 A
nco signal index  123  from row number  123  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.0 177.7 18.24 A
nco signal index  132  from row number  132  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 178.4 54.7 A
nco signal index  133  from row number  133  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 178.4 18.0 A
nco signal index  137  from row number  137  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  118.9 179.3 66.8 V26
nco signal index  142  from row number  142  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.9 179.1 59.24 Q
nco signal index  143  from row number  143  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.9 179.1 28.07 Q
nco signal index  152  from row number  152  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  121.1 180.5 54.86 A83
nco signal index  153  from row number  153  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  121.1 180.5 18.37 A83
nco signal index  161  from row number  161  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  115.3 178.1 64.4 P
nco signal index  170  from row number  170  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  117.9 173.8 44.8 G
nco signal index  182  from row number  182  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  113.6 172.8 66.3 T
nco signal index  205  from row number  205  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  118.4 178.6 64.9 V
nco signal index  209  from row number  209  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  115.7 177.5 64.42 P
nco signal index  213  from row number  213  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.6 177.2 59.94 Q
nco signal index  214  from row number  214  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.6 177.2 28.76 Q
nco signal index  231  from row number  231  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  122.5 178.1 67.24 V
nco signal index  232  from row number  232  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  122.5 178.1 32.07 V
nco signal index  233  from row number  233  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 181.8 54.92 A
nco signal index  234  from row number  234  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 181.8 18.99 A
nco signal index  237  from row number  237  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  124.7 177.1 66.3 T
nco signal index  245  from row number  245  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.5 178.4 58.1 L
nco signal index  246  from row number  246  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.5 178.4 41.7 L
nco signal index  257  from row number  257  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  123.0 178.0 67.2 V
nco signal index  258  from row number  258  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  123.0 178.0 32.12 V
nco signal index  265  from row number  265  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.7 176.1 52.0 A
nco signal index  266  from row number  266  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.7 176.1 19.7 A
nco signal index  271  from row number  271  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  134.5 171.4 44.16 G62
nco signal index  272  from row number  272  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.5 179.2 64.8 P
nco signal index  277  from row number  277  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.2 176.6 54.6 D
nco signal index  278  from row number  278  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.2 176.6 41.2 D
nco signal index  279  from row number  279  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.0 177.1 66.1 I
nco signal index  280  from row number  280  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.0 177.1 38.1 I
nco signal index  308  from row number  308  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.3 178.3 58.07 L
nco signal index  309  from row number  309  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.3 178.3 41.7 L
nco signal index  310  from row number  310  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.1 177.1 66.04 I
nco signal index  311  from row number  311  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.1 177.1 38.13 I
nco signal index  318  from row number  318  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  103.1 177.5 59.95 E
nco signal index  319  from row number  319  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  103.1 177.5 29.06 E
nco signal index  334  from row number  334  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.1 176.3 61.2 R
nco signal index  340  from row number  340  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  121.2 176.1 31.8 V
nco signal index  360  from row number  360  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  115.7 178.2 66.85 P
nco signal index  361  from row number  361  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  115.7 178.2 32.28 P
nco signal index  372  from row number  372  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.5 177.2 65.97 I
nco signal index  373  from row number  373  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.5 177.2 38.13 I
nco signal index  374  from row number  374  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  114.2 177.4 60.52 R
nco signal index  375  from row number  375  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  114.2 177.4 31.4 R
nco signal index  390  from row number  390  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  103.3 178.4 65.9 P
nco signal index  401  from row number  401  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.2 177.2 65.97 P
nco signal index  402  from row number  402  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  119.9 178.5 58.04 L
nco signal index  403  from row number  403  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  119.9 178.5 41.7 L
In summary, the nco signal usage for matching nca asgn is described below:
there are  305  nco signals used for matching nca asgn within their specified degeneracy range.
there are  19  nco signals are never used to match any nca asgn.
there are  74  nco signals are used over their allowed degeneracy number to match nca asgns.
