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Fig. S1. X-ray diffraction patterns of SiBiB-3 at different temperatures.
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Fig. S2. EDX results of BiSiB-3 sample.
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Fig. S3. BiSiB-3 photocatalytic activities toward degrading RhB solution under different temperature.
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Fig. S4. SEM image of BiSiB-3 on the photocatalytic removal of RhB.
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Fig. S5. The Mott-Schottky plots of β-Bi2O3 (a) and Bi2SiO5 (b).
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