
Highlights:

· Electronic waste accumulation poses a significant global issue.

· Supercritical carbon dioxide boosts silver metal extraction efficiency from PCBs.

· Supercritical water pretreatment improves silver accessibility within PCBs.

· Response surface method and thermodynamic modeling optimize the extraction process.

· Results suggest the possibility of designing a larger extraction unit for valuable silver from e-waste.
