Infection control with antimicrobial solid-state ZnO nanoparticles on silk fibroin gauze
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Figure S1. EDS spectrum of ZnO-SF silk fibroin gauze
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Figure S2. Standard curve for zinc ions release measurement
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