TABLE 1S. Substrate moisture content obtained at each change tension. A tension table was used to determine tensions up to 30 kPa while for the others, a potentiometer.
	Tension (kPa)
	Humidity (m3.m-3)

	0
	0,3245

	3
	0,1965

	6
	0,1556

	10
	0,1372

	30
	0,1177

	280
	0,0445

	500
	0,0395

	1000
	0,0343

	1500
	0,0316

	
	

	d =
	1,3000




