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Figure S.1 - Cross-sectional SEM image of 0.5 MB:PVDF and 0.75 MB:PVDF membranes, respectively. 
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Figure S.2 – Diagram of Fe(III) speciation in NaCL 0.7 mol L-1and H3PO4 dissociation.
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