A higher performance agent was synthesized through two-step modification. 

• SDS/isep had a rougher surface and higher porosity. 

• The maximum adsorption capacity of SDS/isep for Pb2+ was 49.1 mg g-1. 

• Adsorption Mechanisms: Electrostatic attraction, ion exchange, complexation, precipitation.
