· High-speed cutting experiments are carried out for Ti-6Al-4V from 0.05 m/s to 86.5 m/s.

· Optimized J-C parameters accurately describe the plastic behavior of Ti-6Al-4V in HSM.
· The formation mechanism of the discontinuously segmented chip is revealed.
· Three distinct cracks form successively during the segmented chip formation process.
