Appendix 
Five-phase induction motor parameters [24]: 
[bookmark: _GoBack]Iphr=2.1 A, 2-poles, 50 Hz, Vphr=220-V, J=0.03 kg.m2, Rs=10 Ω, Rr=6.3 Ω, Lls = 0.04 H,                       Llr= 0.04 H, 
M = 0.42 H. All values are referred to the stator.
PV-array parameters:
The PV-module used is the KC200GT. It has a maximum power output 200 W. The ratings and parameters of the module KC200GT are given in [25]. The PV-array consists of one string which contains nine series connected modules. 

