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Figure S1 Detailed infrared characterization maps of three separators. 1. The polypropylene separator modified with attapulgite nanoparticles based on the surface covalent reaction method. 2. The polypropylene separator modified with attapulgite nanoparticles based on the adsorption method. 3. The original polypropylene separator.
