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1) Cu/stainless steel (SS) composite thin strips with 0.24mm thickness were prepared by a two-pass cold rolling process with intermediate annealing.
2) The interfacial status and the deformation behaviors were effectively controlled by the intermediate annealing.
3) Appropriate intermediate annealing (1000℃) could effectively improve the bonding strength and ductility of the Cu/SS thin strips.
4) The bonding mechanisms are systematically discussed.
