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Fig. S1 SEM image of CP-AC-700 at 10000X.
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Fig. S2 (a-c) TEM images of CP-AC-700; (d-f) HRTEM images of CP-AC-700.
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Fig. S3 Cyclic voltammetry curves of CP-AC-800 in a three-electrode system with 6 M KOH electrolyte.
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Fig. S4 (a) Plot of constant current charge/discharge curves of CP-AC-800 at different current densities.
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