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Fig. S1. Live observation of mussel surface exploration behavior and thread secretion on PVC and PVC/(PDA/PEI)-TA surfaces.
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