V1/A2
Layer Resistivity   Thickness
 1     1628.933       1.020		1.0
 2      330.616       1.748		2.7
 3      311.220       7.937		10.6
 4      638.148      16.131		26.7
 5     1533.333

V2/A3
Layer  Resistivity   Thickness
 1     2688.054       2.311		2.3
 2      593.561      59.346		61.6
 3     5312.750

V3/A4
Layer  Resistivity   Thickness
 1     2057.759       0.403		0.4
 2      682.285       5.106		5.5
 3       53.266       3.196		8.7
 4     1872.198

V4/B6
Layer	 Resistivity	Thickness   Depth
1    	 363.638      	 1.084		1.1
 2     	84.570     	3.841		4.9
 3   	212.614     	5.056		10.0
 4    	50.472     	9.877		19.9
 5  		  14291.999	

V5/C2
Layer  Resistivity   Thickness
 1     2013.097       0.353		0.4
 2      548.129       7.427		7.8
 3       89.486       7.249		15.0
 4    79674.148

V6/B4
Layer  Resistivity   Thickness
 1     1120.438       1.733		1.7
 2      335.602      17.553		19.2
 4      609.866

V7/C6
Layer	 Resistivity 	Thickness     Depth 
1      	187.84      	 2.7		2.7
 2     	 37.092      	 4.202		6.9
 3     	120.123      	7.377		14.3
 4  	 6068.560

V8/C1
Layer  Resistivity   Thickness
 1      189.241       2.063	2.1
 2      304.958      26.388	28.4
 3      536.275       4.876	33.3
 4    15655.978

V9/D3
1      370.467       6.384	6.4
 2      211.557      20.641	27
 3     1350.629

V10/B1
Layer  Resistivity   Thickness
 1      667.890       1.648		1.6
 2     1135.782       4.605		6.2
 3      103.054      12.073		18.2
 4     8962.977
VES11/R4
Layer  Resistivity   Thickness
 1      219.241       2.063	3.1
 2      304.958      26.388	28.4
 3      536.275       4.876	33.3
 4    15655.978

VES12/R3
Layer  Resistivity   Thickness
 1      575.109       5.247            5.0
 2     2561.109       4.641           9.6
 3      162.396      14.491           23.0
 4     3224.069
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	PROFILE 1

	VES Points
	Geologic Layers
	Resistivity (Ωm)
	Thickness (m)
	Depth 
(m)
	Inferred Lithology

	V1
	1
2
3
4
	1629
321
638
1533
	1.0
8.6
16.1
	1.0
10.6
26.7
	Lateritic topsoil
Weathered layer Fractured basement
Fresh basement

	
	
	
	
	
	

	V2
	1
2
3
4
	2058
682
53
1872
	0.4
5.1
3.2
	0.4
5.5
8.7
	Lateritic topsoil
Weathered layer Fractured basement
Fresh basement

	
	
	
	
	
	

	V3
	1
2
3
4
5
	364
85
212
50
14292
	1.1
3.8
5.1
9.9
	1.1
4.9
10
19.9
	Lateritic topsoil
Silty/sand
clay
Weathered layer
Fresh basement

	
	
	
	
	
	

	V4
	1
2
3
4
	2013
548
89
79674
	0.4
7.4
7.2
	0.4
7.8
15
	Lateritic topsoil
Clay/laterite
Weathered layer
Fresh basement

	
	
	
	
	
	

	V5
	1
2
3
4
	188
37
120
6069
	2.7
4.2
7.4
	2.7
6.9
14.3
	Topsoil
Silty/sand/clay
Weathered layer
Fresh basement

	
	
	
	
	
	

	V6
	1
2
3
4
	189
305
536
15656
	2.1
26.3
4.9
	2.1
28.4
33.3
	Topsoil
Weathered layer
Fractured basement Fresh basement

	
	
	
	
	
	

	V7
	1
2
3
4
	668
1136
103
15655
	1.6
4.6
12.1
	1.6
6.2
18.4
	Topsoil
Weathered layer
Fractured basement Fresh basement

	
	
	
	
	
	

	V8
	1
2
3
4
	219
301
536
15656
	3.1
26
5
	3.1
29.1
34.1
	Topsoil
Weathered layer
Fractured basement Fresh basement

	
	
	
	
	
	

	V9
	1
2
3
4
	575
2561
162
3224
	5.2
4.6
14.5
	5.2
9.8
23.3
	Topsoil
Weathered layer
Fractured basement Fresh basement
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	PROFILE 1

	VES Points
	Geologic Layers
	Resistivity (Ωm)
	Thickness (m)
	Depth 
(m)
	Inferred Lithology

	V1
	1
	1629
	1.0
	1.0
	Lateritic topsoil

	
	2
	321
	8.6
	10.6
	Weathered layer

	
	3
	638
	16.1
	26.7
	Fractured basement

	
	4
	1533
	
	
	Fresh basement

	
	
	
	
	
	

	V2
	1
	2688
	2.3
	2.3
	Lateritic topsoil

	
	2
	594
	59.3
	61.6
	Fractured basement

	
	3
	5313
	
	
	Fresh basement

	
	
	
	
	
	

	V3
	1
	2058
	0.4
	0.4
	Lateritic topsoil

	
	2
	682
	5.1
	5.5
	Weathered laterite

	
	3
	53
	3.2
	8.7
	Weathered layer

	
	4
	1872
	
	
	Fresh basement

	
	
	
	
	
	

	V4
	1
	364
	1.1
	1.1
	Topsoil

	
	2
	85
	3.8
	4.9
	Silty/sand

	
	3
	212
	5.1
	10.0
	Clay

	
	4
	50
	9.9
	19.9
	Weathered layer

	
	5
	14292
	
	
	Fresh basement







	PROFILE 2

	VES Points
	Geologic Layers
	Resistivity (Ωm)
	Thickness (m)
	Depth 
(m)
	Inferred Lithology

	V4
	1
	2013
	0.4
	0.4
	Lateritic topsoil

	
	2
	548
	7.4
	7.8
	Weathered laterite

	
	3
	89
	7.2
	15.0
	Weathered layer

	
	4
	79674
	
	
	Fresh basement

	
	
	
	
	
	

	V5
	1
	1120
	1.7
	1.7
	Lateritic topsoil

	
	2
	336
	17.5
	17.2
	Weathered layer

	
	3
	610
	
	
	Fractured basement

	
	
	
	
	
	

	V7
	1
	188
	2.7
	2.7
	Topsoil

	
	2
	37
	4.2
	6.9
	Silty/sand/clay

	
	3
	120
	7.4
	14.3
	Weathered layer

	
	4
	6069
	
	
	Fresh basement



	PROFILE 3

	VES Points
	Geologic Layers
	Resistivity (Ωm)
	Thickness (m)
	Depth 
(m)
	Inferred Lithology

	V8
	1
	189
	2.1
	2.1
	Topsoil

	
	2
	305
	26.3
	28.4
	Weathered layer

	
	3
	536
	4.9
	33.3
	Fractured basement

	
	4
	15656
	
	
	Fresh basement

	
	
	
	
	
	

	V9
	1
	370
	6.4
	6.4
	Topsoil

	
	2
	212
	20.6
	27
	Weathered layer

	
	3
	1351
	
	
	Fresh basement

	
	
	
	
	
	

	V10
	1
	668
	1.6
	1.6
	Topsoil

	
	2
	1136
	4.6
	6.2
	Indurated laterite

	
	3
	103
	12.1
	18.2
	Weathered layer

	
	4
	8963
	
	
	Fresh basement

	
	
	
	
	
	

	V11
	1
	219
	3.1
	3.1
	Topsoil

	
	2
	301
	26.3
	29.4
	Weathered laterite

	
	3
	536
	4.9
	34.3
	Fractured layer

	
	4
	15656
	
	
	Fresh basement

	
	
	
	
	
	

	V12
	1
	575
	5.2
	5.2
	Topsoil

	
	2
	2561
	4.6
	9.8
	Indurated laterite

	
	3
	162
	14.5
	23.3
	Weathered layer

	
	4
	3224
	
	
	Fresh basement
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