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The SLMed porous Inconel718 alloy after homogenizing heat treatment has better mechanical properties due to the precipitation of nano-sized γ" phase.
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