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Figure S1. Schematic diagram of sandstone sampling

Table S1 The classification standard of ultrasonic velocity ratio and weathering grade [47]
	Ultrasonic Velocity ratio
	Grade
	Weathering extent

	0-0.2
	6
	Residual soil

	0.2-0.4
	5
	Fully weathered

	0.4-0.6
	4
	Highly weathered

	0.6-0.8
	3
	Moderately weathered

	0.8-0.9
	2
	Weakly weathered

	0.9-1
	1
	Unweathered
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