1. This paper presents a nonlinear control strategy for a spinning electrodynamic tether system during its spin-up stage;
2. An underactuated controller is proposed to track spinning motion and stabilize tether deformation by adjusting only electrical current.
3. A high-gain saturated controller is proposed to stabilize the attitude motions of end bodies.

