highlights:
· Introducing a novel 1D model approach for optimizing steam ejector entrainment ratio
· new definitions of ejector efficiency
· The main dimensions of an ejector are calculated using the novel 1D model approach
· The maximum theoretical entrainment ratio of an ejector has been validated through CFD simulations
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