1. [bookmark: _GoBack]Enhanced Precision: Achieved enhanced precision, reducing errors to within +/-10um in ISO 10791-6 K1 K2 K4 paths.
2. Rapid Analysis and Compensation: Completed error analysis and compensation in 30 minutes, reducing inspection time by 50%.
3. Comprehensive Error Detection: Enabled multiple error detections using different paths, offering versatile solutions.
4. Commercial Applicability: Validated benefits and reduced setup time showcase high commercial applicability.
5. Optimization of Five-Axis Performance: By compensating across 8 parameters, the simultaneous motion accuracy can be significantly optimized, achieving reductions of up to 10um.
