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Highlights

· The application of zig-zag flow type photocatalytic reactor has been investigated 
· Various catalysts and external oxidants have been investigated
· Hydrogen peroxide-based oxidants found to be best for degradation
· Among catalysts, TiO2 was effective than other catalysts.  
· A zig-zag flow type photocatalytic reactor best alternative to simple photocatalytic reactor 
