· Numerical study examined roughness height's impact on flow variables and turbulence statistics 
· An upper limit on the roughness height-to-water depth ratio for designing steep stepped spillways 
· Profiles of turbulent kinetic energy can be collapsed into one curve for relative roughness <0.8 
· Regardless of the roughness height, maximum velocities in the water column are nearly the same 
