Nco match to nca asgn search completed.
The protein amino acid sequence is:
The protein sequence read from  RSV_seq.txt  is: 
PVVIKTEGPA   WTPLEPKLIT   RLADTVRTKG   LRSPITMAEV   EALMSSPLLP
HDVTNLMRVI   LGPAPYALWM   DAWGVQLQTV   IAAATRDPRH   PANGQGRGER
TNLNRLKGLA   DGMVGNPQGQ   AALLRPGELV   AITASALQAF   REVARLAEPA
GPWADIMQGP   SESFVDFANR   LIKAVEGSDL   PPSARAPVII   DCFRQKSQPD
IQQLIRTAPS   TLTTPGEIIK   YVLDRQKTAP   

The following is the breakdown of sequence composition and residue types in the input nca asignments.
amino acid types             num of copies in sequence         num of copies in ncacx input        num of definitely asgned in ncacx input        num of copies free from local minimum concerns in ncacx input
A            28              28          0          17
C            1              1          0          1
D            11              11          0          11
E            11              11          0          11
F            4              4          0          4
G            16              16          0          16
H            2              2          0          2
I            14              14          0          9
K            8              8          0          8
L            24              24          0          22
M            6              6          0          4
N            6              6          0          4
P            23              23          0          11
Q            12              12          0          8
R            17              17          0          15
S            10              10          0          10
T            16              16          0          11
V            15              15          0          10
W            4              4          0          4
Y            2              2          0          2


Input statistics:
There are  0  sequentially assigned nca asgn pre-existing in ncacx input
There are additional  230  none definite nca asgn.
There are  627  individual resonances(peaks) from ncocx input.
There are  211 individual nco resonances(peaks) not used for match finding.


Matching results:
There are  18  nca inputs do not have matched nco
There are  96 nca inputs have 1 unique matched nco
There are  39  nca inputs have 2 matched nco
There are  21  nca inputs have 3 matched nco
There are  16  nca inputs have 4 matched nco
There are  12  nca inputs have 5 matched nco
There are  49  nca inputs have non-overlaping and unique nco match.
There are additional  19  nca inputs have non-overlaping and non unique nco match.


Overlaping definition: if any nco signals used in a match is used more than 
its specified degeneracy values in the entire nco to nca match search process.
################################################################
There are  18 ncacx inputs with no nco matches, and they are:
ncacx row  1 1000000.0 1000000.0  1000000.0  1000000.0  1 P
ncacx row  9 134.8 1000000.0  64.3  31.72  1 P
ncacx row  11 1000000.0 1000000.0  1000000.0  1000000.0  1 W
ncacx row  15 123.6 1000000.0  54.29  30.2  1 E
ncacx row  21 121.4 178.5  59.6  30.07  1 R
ncacx row  46 118.8 1000000.0  56.0  64.21  1 S
ncacx row  47 140.4 176.2  64.58  32.29  1 P
ncacx row  87 116.6 1000000.0  49.57  42.67  1 D
ncacx row  90 124.4 172.8  57.1  32.17  1 H
ncacx row  116 112.4 172.1  49.8  38.5  1 N
ncacx row  125 123.1 176.6  54.43  30.32  1 R
ncacx row  150 1000000.0 1000000.0  1000000.0  1000000.0  1 A
ncacx row  164 124.5 177.1  63.13  39.3  1 F
ncacx row  180 122.4 1000000.0  54.92  42.92  1 L
ncacx row  192 118.5 1000000.0  56.76  27.2  1 C
ncacx row  208 125.0 1000000.0  50.4  22.44  1 A
ncacx row  226 118.5 1000000.0  59.2  29.4  1 Q
ncacx row  229 1000000.0 1000000.0  1000000.0  1000000.0  1 A
################################################################
We find  96  ncacx inputs have a unique matched nco residue type assignments:
ncacx row  2 121.9 175.3  61.81  34.98  1 V
its nco match is 
125.4 175.1  61.9  34.7

ncacx row  3 125.4 174.0  59.56  35.01  1 V
its nco match is 
125.4 173.8  59.5  35.0

ncacx row  4 125.4 175.9  60.99  36.2  1 I
its nco match is 
128.6 175.7  61.0  36.3

ncacx row  5 128.6 178.5  54.97  34.18  1 K
its nco match is 
116.7 178.5  54.86  33.91

ncacx row  7 125.7 1000000.0  54.9  32.16  1 E
its nco match is 
127.6 176.5  54.94  32.21

ncacx row  12 124.7 170.2  57.26  71.06  1 T
its nco match is 
137.8 170.1  57.1  71.0

ncacx row  13 138.0 176.7  61.7  1000000.0  1 P
its nco match is 
122.7 176.7  62.0

ncacx row  14 122.8 1000000.0  54.9  43.0  1 L
its nco match is 
123.7 177.0  54.9  43.0

ncacx row  18 119.6 1000000.0  57.4  41.62  1 L
its nco match is 
119.9 178.5  57.4  41.62

ncacx row  19 119.8 178.6  64.61  37.84  1 I
its nco match is 
117.7 178.6  64.9  37.63

ncacx row  22 121.6 178.3  57.78  42.1  1 L
its nco match is 
122.2 178.3  57.78  42.1

ncacx row  27 118.7 177.9  59.56  30.74  1 R
its nco match is 
107.9 177.9  59.56  30.74

ncacx row  28 107.8 176.6  63.88  70.4  1 T
its nco match is 
119.8 176.4  63.9  70.4

ncacx row  31 120.3 1000000.0  55.63  43.0  1 L
its nco match is 
113.1 176.0  55.63  43.0

ncacx row  32 112.8 176.6  55.46  31.13  1 R
its nco match is 
113.8 176.6  55.46  31.13

ncacx row  35 119.1 1000000.0  60.5  38.1  1 I
its nco match is 
118.5 176.6  60.2  38.4

ncacx row  37 118.3 1000000.0  57.84  32.47  1 M
its nco match is 
120.3 177.6  57.74  32.25

ncacx row  41 119.0 179.2  60.5  30.07  1 E
its nco match is 
119.8 179.2  60.47  29.99

ncacx row  43 120.2 178.0  58.26  42.1  1 L
its nco match is 
114.2 178.0  58.26  42.1

ncacx row  44 114.3 174.7  55.68  33.64  1 M
its nco match is 
112.6 174.7  55.55  33.8

ncacx row  48 125.0 174.4  53.85  45.0  1 L
its nco match is 
112.8 174.4  53.85  45.0

ncacx row  49 112.5 174.9  52.38  41.2  1 L
its nco match is 
137.2 174.9  52.38  41.2

ncacx row  55 118.6 176.1  57.4  38.76  1 N
its nco match is 
120.2 175.9  57.7  38.74

ncacx row  57 114.7 1000000.0  56.4  30.56  1 M
its nco match is 
118.5 177.3  56.6  30.88

ncacx row  61 118.7 1000000.0  52.98  44.17  1 L
its nco match is 
103.2 177.1  52.98  44.17

ncacx row  66 118.8 1000000.0  62.46  38.25  1 Y
its nco match is 
122.7 176.7  62.3  38.2

ncacx row  74 103.8 176.2  47.73  1000000.0  1 G
its nco match is 
122.1 176.1  47.71

ncacx row  80 125.4 177.4  66.06  31.03  1 V
its nco match is 
118.7 177.3  66.1  30.9

ncacx row  81 118.5 1000000.0  63.2  35.95  1 I
its nco match is 
124.5 178.9  63.24  36.05

ncacx row  84 120.8 1000000.0  53.16  17.42  1 A
its nco match is 
113.9 178.8  53.38  17.46

ncacx row  85 113.8 174.8  65.35  69.1  1 T
its nco match is 
119.5 175.0  65.4  69.1

ncacx row  86 119.4 175.7  57.54  31.08  1 R
its nco match is 
116.5 175.7  57.54  31.08

ncacx row  88 139.4 178.1  64.5  32.9  1 P
its nco match is 
115.3 178.1  64.4  32.9

ncacx row  89 115.1 175.7  55.64  29.44  1 R
its nco match is 
124.6 175.7  55.64  29.44

ncacx row  95 118.3 177.8  56.5  29.66  1 Q
its nco match is 
108.6 177.8  56.37  29.78

ncacx row  97 119.6 176.7  57.54  31.08  1 R
its nco match is 
112.4 176.7  57.54  31.08

ncacx row  100 121.3 178.5  55.34  31.49  1 R
its nco match is 
117.7 178.5  55.34  31.49

ncacx row  101 117.7 172.8  63.34  66.36  1 T
its nco match is 
113.6 172.8  63.0  66.3

ncacx row  102 113.3 174.3  53.5  40.2  1 N
its nco match is 
120.2 174.2  53.2  40.2

ncacx row  103 120.2 177.2  58.3  42.4  1 L
its nco match is 
115.0 177.1  58.3  42.4

ncacx row  104 115.0 178.5  56.1  37.0  1 N
its nco match is 
120.7 178.5  56.1  37.0

ncacx row  105 120.6 177.8  60.7  31.1  1 R
its nco match is 
113.2 177.8  60.7  31.1

ncacx row  106 113.3 175.2  57.1  41.4  1 L
its nco match is 
108.0 175.2  57.1  41.4

ncacx row  107 107.7 177.8  56.4  34.4  1 K
its nco match is 
108.3 177.8  56.4  34.4

ncacx row  108 108.6 174.0  46.9  1000000.0  1 G
its nco match is 
115.8 173.9  46.7

ncacx row  109 115.7 176.4  53.9  43.6  1 L
its nco match is 
121.5 176.4  53.9  43.6

ncacx row  110 121.4 175.9  50.9  19.6  1 A
its nco match is 
120.1 176.1  50.6  19.6

ncacx row  111 119.9 176.8  57.0  40.7  1 D
its nco match is 
112.1 176.9  56.8  40.7

ncacx row  113 113.3 177.4  57.3  34.6  1 M
its nco match is 
121.6 177.2  57.1  34.6

ncacx row  114 121.4 178.6  64.9  31.0  1 V
its nco match is 
118.4 178.6  64.9  30.9

ncacx row  115 118.1 174.7  46.5  1000000.0  1 G
its nco match is 
112.2 174.6  46.39

ncacx row  122 117.1 180.0  54.0  18.9  1 A
its nco match is 
115.3 180.0  53.9  19.1

ncacx row  123 115.3 179.1  56.59  45.8  1 L
its nco match is 
120.2 179.1  56.59  45.8

ncacx row  124 120.3 1000000.0  55.63  42.77  1 L
its nco match is 
123.3 176.9  55.63  42.77

ncacx row  127 102.3 178.4  46.65  1000000.0  1 G
its nco match is 
119.7 178.6  46.59

ncacx row  128 119.4 176.2  60.3  29.13  1 E
its nco match is 
117.8 176.2  60.52  29.14

ncacx row  129 117.9 180.8  58.2  41.33  1 L
its nco match is 
120.5 180.8  58.2  41.33

ncacx row  131 122.6 181.6  54.99  19.04  1 A
its nco match is 
123.3 181.8  54.92  18.99

ncacx row  132 123.1 177.9  66.83  39.8  1 I
its nco match is 
117.6 178.0  66.85  39.66

ncacx row  134 124.8 182.2  55.5  18.26  1 A
its nco match is 
113.5 182.2  55.54  18.23

ncacx row  135 113.2 176.2  62.61  63.48  1 S
its nco match is 
125.9 176.2  62.8  63.3

ncacx row  136 126.0 1000000.0  56.26  20.56  1 A
its nco match is 
122.3 180.5  56.32  20.58

ncacx row  137 122.2 178.4  58.14  41.7  1 L
its nco match is 
119.5 178.4  58.14  41.7

ncacx row  139 126.4 1000000.0  55.3  20.6  1 A
its nco match is 
119.0 177.3  55.45  20.8

ncacx row  141 119.0 177.2  60.58  29.86  1 R
its nco match is 
117.3 177.2  60.58  29.86

ncacx row  142 117.5 176.3  59.5  28.1  1 E
its nco match is 
121.9 176.3  59.6  28.3

ncacx row  144 123.0 177.1  55.1  17.12  1 A
its nco match is 
113.2 177.1  54.9  17.4

ncacx row  145 113.3 179.3  58.5  30.46  1 R
its nco match is 
119.2 179.3  58.5  30.46

ncacx row  146 119.2 177.1  56.4  43.34  1 L
its nco match is 
123.3 177.1  56.4  43.34

ncacx row  153 119.3 1000000.0  62.9  28.6  1 W
its nco match is 
124.5 178.9  63.24  28.85

ncacx row  158 126.7 178.8  56.2  27.81  1 Q
its nco match is 
120.7 178.5  56.1  27.7

ncacx row  161 112.6 173.1  56.81  63.7  1 S
its nco match is 
125.8 173.0  56.9  63.75

ncacx row  162 125.7 176.7  54.93  32.19  1 E
its nco match is 
127.6 176.5  54.94  32.21

ncacx row  163 127.4 175.1  58.36  64.23  1 S
its nco match is 
124.2 175.1  58.31  64.16

ncacx row  166 121.3 179.3  58.26  39.96  1 D
its nco match is 
123.3 179.1  58.26  39.91

ncacx row  167 123.3 175.4  59.21  39.06  1 F
its nco match is 
121.9 175.5  59.31  38.98

ncacx row  169 115.2 179.3  56.56  38.09  1 N
its nco match is 
120.6 179.3  56.5  37.8

ncacx row  170 120.6 177.8  60.73  31.1  1 R
its nco match is 
122.2 177.8  60.73  31.1

ncacx row  171 122.2 1000000.0  58.14  41.7  1 L
its nco match is 
119.5 178.4  58.14  41.7

ncacx row  181 138.0 175.9  61.64  1000000.0  1 P
its nco match is 
135.9 175.9  61.3

ncacx row  183 110.3 174.8  60.48  62.62  1 S
its nco match is 
122.2 174.7  60.41  62.59

ncacx row  185 115.8 176.4  61.0  30.35  1 R
its nco match is 
119.1 176.4  61.0  30.35

ncacx row  193 118.5 1000000.0  62.0  39.5  1 F
its nco match is 
116.4 177.7  61.9  39.4

ncacx row  194 116.3 178.1  60.05  31.71  1 R
its nco match is 
113.2 178.1  60.05  31.71

ncacx row  197 113.1 1000000.0  57.29  65.05  1 S
its nco match is 
121.0 177.2  57.05  64.95

ncacx row  200 115.9 178.6  57.15  39.33  1 D
its nco match is 
123.4 178.6  57.4  39.31

ncacx row  201 123.4 178.3  62.57  36.27  1 I
its nco match is 
119.5 178.4  62.47  36.16

ncacx row  206 119.8 1000000.0  60.45  31.18  1 R
its nco match is 
114.2 177.4  60.45  31.18

ncacx row  211 117.2 175.5  68.1  69.0  1 T
its nco match is 
124.7 175.5  68.21  69.2

ncacx row  212 124.5 1000000.0  53.7  44.7  1 L
its nco match is 
111.7 174.4  53.7  44.7

ncacx row  213 111.8 174.5  62.9  71.0  1 T
its nco match is 
110.1 174.2  62.69  70.9

ncacx row  214 110.3 173.3  58.14  69.82  1 T
its nco match is 
131.8 173.2  58.5  69.8

ncacx row  218 121.1 1000000.0  62.56  37.09  1 I
its nco match is 
120.4 178.2  62.47  37.03

ncacx row  223 119.1 1000000.0  58.03  41.4  1 L
its nco match is 
119.9 178.5  58.03  41.4

ncacx row  224 119.6 1000000.0  56.88  40.62  1 D
its nco match is 
112.1 176.9  56.8  40.7

ncacx row  230 140.6 1000000.0  64.6  32.3  1 P
its nco match is 
119.2 178.8  64.86  32.0

################################################################
We find  39  ncacx inputs have 2 matched nco residue type assignments:
ncacx row  6 116.5 1000000.0  59.21  65.96  1 T
its first nco match is 
117.2 173.5  59.16  65.95

its 2nd nco match is 
116.9 173.4  59.1  65.8

ncacx row  10 123.1 1000000.0  52.05  20.1  1 A
its first nco match is 
120.7 176.1  52.0  19.7

its 2nd nco match is 
115.7 177.7  52.09  20.07

ncacx row  24 119.6 1000000.0  57.3  40.62  1 D
its first nco match is 
122.3 178.7  57.56  40.82

its 2nd nco match is 
122.3 178.5  57.4  40.8

ncacx row  29 120.0 1000000.0  55.71  32.59  1 K
its first nco match is 
107.7 178.0  55.61  32.5

its 2nd nco match is 
136.9 175.5  55.82  32.78

ncacx row  45 112.5 1000000.0  60.43  63.71  1 S
its first nco match is 
118.9 174.9  60.4  63.7

its 2nd nco match is 
118.9 174.9  60.4  63.62

ncacx row  52 115.9 1000000.0  57.2  39.4  1 D
its first nco match is 
115.4 178.2  57.4  39.8

its 2nd nco match is 
123.4 178.6  57.4  39.31

ncacx row  53 115.6 1000000.0  66.07  31.93  1 V
its first nco match is 
112.2 176.7  65.88  32.14

its 2nd nco match is 
110.2 179.1  66.4  32.27

ncacx row  56 120.2 1000000.0  58.3  42.4  1 L
its first nco match is 
114.6 177.9  58.3  42.4

its 2nd nco match is 
115.0 177.1  58.3  42.4

ncacx row  58 118.5 1000000.0  59.2  28.2  1 R
its first nco match is 
115.7 178.9  59.35  28.5

its 2nd nco match is 
116.9 179.1  59.24  28.07

ncacx row  60 109.2 175.1  63.53  39.07  1 I
its first nco match is 
118.9 174.9  63.7  38.9

its 2nd nco match is 
118.8 174.8  63.62  38.9

ncacx row  68 118.3 1000000.0  56.4  43.34  1 L
its first nco match is 
121.5 176.3  56.4  43.34

its 2nd nco match is 
123.3 177.1  56.4  43.34

ncacx row  71 119.9 1000000.0  57.1  40.7  1 D
its first nco match is 
122.3 178.5  57.4  40.8

its 2nd nco match is 
112.1 176.9  56.8  40.7

ncacx row  73 123.3 1000000.0  59.7  26.97  1 W
its first nco match is 
119.8 179.3  60.0  27.25

its 2nd nco match is 
103.5 177.5  59.95  26.96

ncacx row  77 120.2 1000000.0  58.29  42.4  1 L
its first nco match is 
118.3 179.7  58.29  42.4

its 2nd nco match is 
115.0 177.1  58.3  42.4

ncacx row  78 118.5 1000000.0  59.14  28.01  1 Q
its first nco match is 
116.9 179.1  59.24  28.07

its 2nd nco match is 
119.3 178.9  59.3  27.75

ncacx row  92 122.6 1000000.0  54.99  19.04  1 A
its first nco match is 
117.1 177.8  54.92  19.04

its 2nd nco match is 
123.3 181.8  54.92  18.99

ncacx row  93 117.1 1000000.0  54.54  41.07  1 N
its first nco match is 
121.2 176.6  54.6  41.2

its 2nd nco match is 
122.4 177.9  54.8  40.8

ncacx row  96 108.6 173.8  44.1  1000000.0  1 G
its first nco match is 
120.0 173.9  44.4

its 2nd nco match is 
119.9 173.8  44.3

ncacx row  117 139.4 177.5  64.5  1000000.0  1 P
its first nco match is 
122.8 177.1  64.5

its 2nd nco match is 
115.7 177.5  64.42

ncacx row  118 115.5 179.2  59.71  26.96  1 Q
its first nco match is 
119.8 179.3  60.0  27.25

its 2nd nco match is 
109.3 179.1  60.13  26.95

ncacx row  119 109.2 176.0  46.89  1000000.0  1 G
its first nco match is 
119.5 175.8  47.08

its 2nd nco match is 
119.7 175.9  47.1

ncacx row  121 118.9 180.2  54.79  18.5  1 A
its first nco match is 
121.1 180.5  54.86  18.37

its 2nd nco match is 
117.1 180.0  54.6  18.38

ncacx row  148 137.5 1000000.0  50.1  28.01  1 E
its first nco match is 
136.6 177.7  49.8  28.0

its 2nd nco match is 
110.2 179.1  49.87  27.95

ncacx row  154 123.0 1000000.0  55.2  17.1  1 A
its first nco match is 
113.2 177.1  54.9  17.4

its 2nd nco match is 
117.0 181.5  55.3  17.1

ncacx row  155 117.1 1000000.0  54.5  41.1  1 D
its first nco match is 
121.2 176.6  54.6  41.2

its 2nd nco match is 
122.4 177.9  54.8  40.8

ncacx row  160 135.0 177.8  65.13  31.69  1 P
its first nco match is 
109.2 177.7  65.52  32.05

its 2nd nco match is 
112.5 177.8  64.93  31.67

ncacx row  168 122.0 177.8  54.58  18.2  1 A
its first nco match is 
118.0 177.7  54.92  18.24

its 2nd nco match is 
115.3 177.8  54.61  18.5

ncacx row  176 120.8 177.6  60.08  29.09  1 E
its first nco match is 
118.6 177.2  59.94  28.76

its 2nd nco match is 
103.1 177.5  59.95  29.06

ncacx row  177 103.0 174.0  44.96  1000000.0  1 G
its first nco match is 
117.9 173.8  44.8

its 2nd nco match is 
117.9 173.8  44.94

ncacx row  178 117.7 173.4  58.93  65.83  1 S
its first nco match is 
117.2 173.5  59.16  65.95

its 2nd nco match is 
116.9 173.4  59.1  65.8

ncacx row  179 117.0 1000000.0  54.55  41.04  1 D
its first nco match is 
121.2 176.6  54.6  41.2

its 2nd nco match is 
122.4 177.9  54.8  40.8

ncacx row  187 131.7 179.3  66.03  1000000.0  1 P
its first nco match is 
110.2 179.1  66.4

its 2nd nco match is 
117.5 179.3  65.96

ncacx row  191 121.2 1000000.0  58.08  40.2  1 D
its first nco match is 
123.3 179.1  58.26  39.91

its 2nd nco match is 
118.5 179.8  58.2  40.4

ncacx row  195 113.0 1000000.0  57.34  32.14  1 Q
its first nco match is 
120.3 177.6  57.74  32.25

its 2nd nco match is 
114.9 177.9  57.1  32.3

ncacx row  196 115.1 1000000.0  55.64  29.44  1 K
its first nco match is 
124.6 175.7  55.64  29.44

its 2nd nco match is 
113.1 177.4  55.63  29.51

ncacx row  198 121.0 1000000.0  55.75  28.4  1 Q
its first nco match is 
113.1 176.0  55.63  28.35

its 2nd nco match is 
136.9 175.5  55.82  28.1

ncacx row  203 115.7 1000000.0  60.97  27.89  1 Q
its first nco match is 
119.1 176.4  61.0  27.86

its 2nd nco match is 
120.7 178.5  60.6  27.7

ncacx row  204 120.9 1000000.0  58.04  42.39  1 L
its first nco match is 
115.0 177.1  58.3  42.4

its 2nd nco match is 
118.8 179.3  58.04  42.39

ncacx row  210 117.4 173.4  58.9  65.8  1 S
its first nco match is 
117.2 173.5  59.16  65.95

its 2nd nco match is 
116.9 173.4  59.1  65.8

################################################################
We find  21  ncacx inputs have 3 matched nco residue type assignments:
ncacx row  8 107.7 171.5  44.3  1000000.0  1 G
its first nco match is 
134.5 171.3  44.16

its 2nd nco match is 
134.8 171.3  44.12

its 3rd nco match is 
134.5 171.4  44.16

ncacx row  30 107.7 173.8  44.46  1000000.0  1 G
its first nco match is 
120.0 173.9  44.4

its 2nd nco match is 
117.9 173.8  44.8

its 3rd nco match is 
119.9 173.8  44.3

ncacx row  51 116.2 1000000.0  60.34  31.29  1 H
its first nco match is 
118.6 177.2  59.94  30.88

its 2nd nco match is 
118.6 177.2  59.94  30.9

its 3rd nco match is 
114.2 177.4  60.45  31.18

ncacx row  62 103.2 171.4  44.35  1000000.0  1 G
its first nco match is 
134.5 171.3  44.16

its 2nd nco match is 
134.8 171.3  44.12

its 3rd nco match is 
134.5 171.4  44.16

ncacx row  63 134.8 179.2  65.0  1000000.0  1 P
its first nco match is 
119.2 178.8  64.86

its 2nd nco match is 
119.2 179.2  64.8

its 3rd nco match is 
119.5 179.2  64.8

ncacx row  69 121.2 1000000.0  57.0  28.4  1 W
its first nco match is 
118.5 177.3  56.6  28.76

its 2nd nco match is 
120.8 177.1  57.11  28.12

its 3rd nco match is 
121.3 177.3  57.11  28.07

ncacx row  70 121.0 1000000.0  57.93  31.23  1 M
its first nco match is 
120.3 177.6  57.74  31.58

its 2nd nco match is 
119.7 179.8  58.2  31.4

its 3rd nco match is 
114.4 176.1  57.76  31.21

ncacx row  94 107.7 173.8  44.5  1000000.0  1 G
its first nco match is 
120.0 173.9  44.4

its 2nd nco match is 
117.9 173.8  44.8

its 3rd nco match is 
119.9 173.8  44.3

ncacx row  99 121.6 1000000.0  57.01  28.4  1 E
its first nco match is 
118.5 177.3  56.6  28.76

its 2nd nco match is 
120.8 177.1  57.11  28.12

its 3rd nco match is 
121.3 177.3  57.11  28.07

ncacx row  112 112.0 174.6  45.1  1000000.0  1 G
its first nco match is 
112.8 174.4  45.0

its 2nd nco match is 
121.7 174.7  44.7

its 3rd nco match is 
113.0 174.6  44.9

ncacx row  130 120.5 178.12  67.25  32.14  1 V
its first nco match is 
122.5 178.1  67.24  32.07

its 2nd nco match is 
123.0 178.0  67.2  32.12

its 3rd nco match is 
115.7 178.2  66.85  32.28

ncacx row  143 121.8 178.0  66.9  31.9  1 V
its first nco match is 
122.5 178.1  67.24  32.07

its 2nd nco match is 
123.0 178.0  67.2  32.12

its 3rd nco match is 
115.7 178.2  66.85  32.28

ncacx row  147 123.1 1000000.0  52.02  20.0  1 A
its first nco match is 
120.1 174.9  51.9  19.62

its 2nd nco match is 
120.7 176.1  52.0  19.7

its 3rd nco match is 
115.7 177.7  52.09  20.07

ncacx row  149 136.6 1000000.0  61.23  1000000.0  1 P
its first nco match is 
128.6 175.7  61.0

its 2nd nco match is 
135.9 175.9  61.3

its 3rd nco match is 
119.1 176.4  61.0

ncacx row  151 107.7 174.0  44.45  1000000.0  1 G
its first nco match is 
120.0 173.9  44.4

its 2nd nco match is 
117.9 173.8  44.8

its 3rd nco match is 
119.9 173.8  44.3

ncacx row  157 118.7 1000000.0  60.51  30.02  1 M
its first nco match is 
119.8 179.2  60.47  29.99

its 2nd nco match is 
117.3 177.2  60.58  29.86

its 3rd nco match is 
126.7 173.7  60.7  30.04

ncacx row  159 119.5 173.4  44.95  1000000.0  1 G
its first nco match is 
117.9 173.8  44.8

its 2nd nco match is 
134.7 173.3  44.88

its 3rd nco match is 
117.9 173.8  44.94

ncacx row  184 122.2 1000000.0  51.9  20.01  1 A
its first nco match is 
120.1 174.9  51.9  19.62

its 2nd nco match is 
120.7 176.1  52.0  19.7

its 3rd nco match is 
115.7 177.7  52.09  20.07

ncacx row  190 117.2 1000000.0  66.6  37.77  1 I
its first nco match is 
117.3 176.8  66.4  37.9

its 2nd nco match is 
120.9 180.2  66.8  37.5

its 3rd nco match is 
117.2 176.3  66.43  37.9

ncacx row  216 103.1 175.9  47.4  1000000.0  1 G
its first nco match is 
122.1 176.1  47.71

its 2nd nco match is 
119.5 175.8  47.08

its 3rd nco match is 
119.7 175.9  47.1

ncacx row  225 118.4 1000000.0  56.4  29.74  1 R
its first nco match is 
108.6 177.8  56.37  29.78

its 2nd nco match is 
119.8 178.8  56.5  29.46

its 3rd nco match is 
118.2 178.4  56.4  29.74

################################################################
We find  16  ncacx inputs have 4 matched nco residue type assignments:
ncacx row  20 117.6 176.2  66.7  68.6  1 T
its first nco match is 
121.2 176.1  67.0  68.3

its 2nd nco match is 
121.6 176.1  67.07  68.27

its 3rd nco match is 
121.3 176.1  67.09  68.3

its 4th nco match is 
121.2 176.1  67.09  68.3

ncacx row  23 122.2 180.9  54.95  17.82  1 A
its first nco match is 
119.5 180.9  54.83  17.9

its 2nd nco match is 
119.8 180.9  54.83  17.8

its 3rd nco match is 
120.0 180.9  54.84  17.9

its 4th nco match is 
122.7 180.5  55.0  17.78

ncacx row  25 122.1 1000000.0  67.21  68.24  1 T
its first nco match is 
121.2 176.1  67.0  68.3

its 2nd nco match is 
121.6 176.1  67.07  68.27

its 3rd nco match is 
121.3 176.1  67.09  68.3

its 4th nco match is 
121.2 176.1  67.09  68.3

ncacx row  34 140.6 178.8  64.58  32.29  1 P
its first nco match is 
119.2 178.8  64.86  32.0

its 2nd nco match is 
119.2 178.8  64.86  32.7

its 3rd nco match is 
119.2 179.2  64.8  32.0

its 4th nco match is 
119.2 179.2  64.8  32.7

ncacx row  54 111.9 176.9  65.83  68.15  1 T
its first nco match is 
118.3 176.7  66.01  68.3

its 2nd nco match is 
118.3 176.7  66.01  68.1

its 3rd nco match is 
118.3 176.7  66.0  68.3

its 4th nco match is 
118.3 176.7  66.0  68.1

ncacx row  59 115.4 1000000.0  65.57  31.83  1 V
its first nco match is 
112.2 176.7  65.88  32.14

its 2nd nco match is 
109.2 177.7  65.52  32.05

its 3rd nco match is 
119.1 177.2  65.97  31.5

its 4th nco match is 
119.2 177.2  65.97  31.5

ncacx row  64 119.2 176.0  57.09  15.49  1 A
its first nco match is 
131.9 176.0  56.99  15.44

its 2nd nco match is 
131.9 176.0  56.99  15.44

its 3rd nco match is 
131.9 176.0  56.99  15.44

its 4th nco match is 
131.9 176.0  56.99  15.44

ncacx row  76 119.0 1000000.0  60.5  29.14  1 Q
its first nco match is 
120.0 179.5  60.47  29.34

its 2nd nco match is 
117.8 176.2  60.52  29.14

its 3rd nco match is 
126.7 173.7  60.7  29.17

its 4th nco match is 
115.7 177.5  60.6  28.79

ncacx row  98 112.1 174.7  45.0  1000000.0  1 G
its first nco match is 
112.8 174.4  45.0

its 2nd nco match is 
121.7 174.7  44.7

its 3rd nco match is 
113.0 174.6  44.9

its 4th nco match is 
111.7 174.4  44.7

ncacx row  120 119.8 177.2  60.2  28.9  1 Q
its first nco match is 
118.6 177.2  59.94  28.76

its 2nd nco match is 
103.1 177.5  59.95  29.06

its 3rd nco match is 
115.7 177.5  60.6  28.79

its 4th nco match is 
114.2 177.4  60.45  28.78

ncacx row  138 119.5 1000000.0  58.3  28.36  1 Q
its first nco match is 
114.2 178.0  58.26  28.13

its 2nd nco match is 
114.6 177.9  58.3  28.23

its 3rd nco match is 
115.0 177.1  58.3  28.15

its 4th nco match is 
126.4 176.1  58.33  28.2

ncacx row  140 119.0 1000000.0  62.98  38.88  1 F
its first nco match is 
118.9 176.1  63.2  39.0

its 2nd nco match is 
118.9 176.1  63.2  39.06

its 3rd nco match is 
118.9 176.1  63.15  39.0

its 4th nco match is 
118.9 176.1  63.15  39.06

ncacx row  182 136.2 1000000.0  66.8  32.41  1 P
its first nco match is 
101.9 179.5  66.62  32.03

its 2nd nco match is 
123.0 178.0  67.2  32.12

its 3rd nco match is 
110.2 179.1  66.4  32.27

its 4th nco match is 
115.7 178.2  66.85  32.28

ncacx row  186 119.2 1000000.0  57.09  15.49  1 A
its first nco match is 
131.9 176.0  56.99  15.44

its 2nd nco match is 
131.9 176.0  56.99  15.44

its 3rd nco match is 
131.9 176.0  56.99  15.44

its 4th nco match is 
131.9 176.0  56.99  15.44

ncacx row  219 120.3 1000000.0  66.49  38.07  1 I
its first nco match is 
119.0 177.1  66.1  38.1

its 2nd nco match is 
119.0 177.1  66.1  38.13

its 3rd nco match is 
117.3 176.8  66.4  37.9

its 4th nco match is 
117.2 176.3  66.43  37.9

ncacx row  221 119.0 1000000.0  62.98  38.88  1 Y
its first nco match is 
118.9 176.1  63.2  39.0

its 2nd nco match is 
118.9 176.1  63.2  39.06

its 3rd nco match is 
118.9 176.1  63.15  39.0

its 4th nco match is 
118.9 176.1  63.15  39.06

################################################################
We find  12  ncacx inputs have five matched nco residue type assignments:
ncacx row  17 116.5 1000000.0  59.7  32.29  1 K
its first nco match is 
119.8 179.3  60.0  31.94

its 2nd nco match is 
118.6 177.2  59.94  32.58

its 3rd nco match is 
119.2 179.0  59.4  32.7

its 4th nco match is 
119.3 178.9  59.3  32.0

its 5th nco match is 
119.3 178.9  59.3  32.7

ncacx row  33 113.9 1000000.0  55.25  64.42  1 S
its first nco match is 
140.3 173.9  55.32  64.36

its 2nd nco match is 
140.3 173.9  55.32  64.36

its 3rd nco match is 
140.2 173.9  55.5  64.36

its 4th nco match is 
140.2 173.9  55.5  64.36

its 5th nco match is 
140.6 173.9  55.35  64.4

ncacx row  36 118.6 1000000.0  66.46  68.64  1 T
its first nco match is 
125.2 177.1  66.4  68.6

its 2nd nco match is 
124.7 177.1  66.3  68.46

its 3rd nco match is 
124.7 177.1  66.3  68.3

its 4th nco match is 
124.7 177.0  66.3  68.46

its 5th nco match is 
124.7 177.0  66.3  68.3

ncacx row  42 120.0 180.9  55.08  18.1  1 A
its first nco match is 
119.5 180.9  54.83  17.9

its 2nd nco match is 
119.8 180.9  54.83  17.8

its 3rd nco match is 
120.0 180.9  54.84  17.9

its 4th nco match is 
122.7 180.5  55.0  17.78

its 5th nco match is 
121.1 180.5  54.86  18.37

ncacx row  65 131.7 1000000.0  65.84  31.7  1 P
its first nco match is 
109.2 177.7  65.52  32.05

its 2nd nco match is 
119.1 177.2  65.97  31.5

its 3rd nco match is 
119.0 177.1  66.1  31.5

its 4th nco match is 
119.1 177.1  66.04  31.5

its 5th nco match is 
119.2 177.2  65.97  31.5

ncacx row  67 122.7 1000000.0  54.86  18.43  1 A
its first nco match is 
118.0 177.7  54.92  18.24

its 2nd nco match is 
121.1 180.5  54.86  18.37

its 3rd nco match is 
117.1 180.0  54.6  18.38

its 4th nco match is 
115.3 177.8  54.61  18.5

its 5th nco match is 
117.5 177.2  54.5  18.5

ncacx row  79 117.1 177.1  66.48  68.69  1 T
its first nco match is 
125.2 177.1  66.4  68.6

its 2nd nco match is 
124.7 177.1  66.3  68.46

its 3rd nco match is 
124.7 177.1  66.3  68.3

its 4th nco match is 
124.7 177.0  66.3  68.46

its 5th nco match is 
124.7 177.0  66.3  68.3

ncacx row  83 122.7 1000000.0  54.86  18.43  1 A
its first nco match is 
118.0 177.7  54.92  18.24

its 2nd nco match is 
121.1 180.5  54.86  18.37

its 3rd nco match is 
117.1 180.0  54.6  18.38

its 4th nco match is 
115.3 177.8  54.61  18.5

its 5th nco match is 
117.5 177.2  54.5  18.5

ncacx row  174 120.9 1000000.0  54.9  18.5  1 A
its first nco match is 
118.0 177.7  54.92  18.24

its 2nd nco match is 
121.1 180.5  54.86  18.37

its 3rd nco match is 
117.1 180.0  54.6  18.38

its 4th nco match is 
115.3 177.8  54.61  18.5

its 5th nco match is 
117.5 177.2  54.5  18.5

ncacx row  222 118.8 1000000.0  66.03  29.95  1 V
its first nco match is 
119.1 177.2  65.97  30.12

its 2nd nco match is 
119.0 177.1  66.1  30.12

its 3rd nco match is 
119.1 177.1  66.04  30.12

its 4th nco match is 
119.5 177.2  65.97  29.97

its 5th nco match is 
119.2 177.2  65.97  30.12

ncacx row  227 119.6 1000000.0  57.78  31.18  1 K
its first nco match is 
120.3 177.6  57.74  31.58

its 2nd nco match is 
119.7 179.8  58.2  31.4

its 3rd nco match is 
116.5 175.7  57.54  31.08

its 4th nco match is 
112.4 176.7  57.54  31.08

its 5th nco match is 
114.4 176.1  57.76  31.21

ncacx row  228 114.4 174.1  55.5  64.66  1 T
its first nco match is 
140.3 173.9  55.32  64.36

its 2nd nco match is 
140.3 173.9  55.32  64.36

its 3rd nco match is 
140.2 173.9  55.5  64.36

its 4th nco match is 
140.2 173.9  55.5  64.36

its 5th nco match is 
140.6 173.9  55.35  64.4

################################################################
The following list the nco signals never used in match finding:
nco signal index  1  from row number  1  in the original ncocx input file is not used.
Its coordn are  121.8 171.3 62.4 P
nco signal index  2  from row number  1  in the original ncocx input file is not used.
Its coordn are  121.8 171.3 32.2 P
nco signal index  3  from row number  1  in the original ncocx input file is not used.
Its coordn are  121.8 171.3 26.5 P
nco signal index  6  from row number  2  in the original ncocx input file is not used.
Its coordn are  125.4 175.1 22.72 P
nco signal index  7  from row number  2  in the original ncocx input file is not used.
Its coordn are  125.4 175.1 21.5 P
nco signal index  10  from row number  3  in the original ncocx input file is not used.
Its coordn are  125.4 173.8 22.69 P
nco signal index  11  from row number  3  in the original ncocx input file is not used.
Its coordn are  125.4 173.8 21.56 P
nco signal index  14  from row number  4  in the original ncocx input file is not used.
Its coordn are  128.6 175.7 27.25 P
nco signal index  15  from row number  4  in the original ncocx input file is not used.
Its coordn are  128.6 175.7 18.2 P
nco signal index  18  from row number  5  in the original ncocx input file is not used.
Its coordn are  116.7 178.5 25.45 P
nco signal index  26  from row number  11  in the original ncocx input file is not used.
Its coordn are  124.4 168.2 27.9 P
nco signal index  29  from row number  12  in the original ncocx input file is not used.
Its coordn are  137.8 170.1 20.65 P
nco signal index  33  from row number  14  in the original ncocx input file is not used.
Its coordn are  123.7 177.0 27.56 P
nco signal index  34  from row number  15  in the original ncocx input file is not used.
Its coordn are  139.1 176.2 54.97 P
nco signal index  35  from row number  15  in the original ncocx input file is not used.
Its coordn are  139.1 176.2 30.4 P
nco signal index  36  from row number  15  in the original ncocx input file is not used.
Its coordn are  139.1 176.2 36.85 P
nco signal index  40  from row number  17  in the original ncocx input file is not used.
Its coordn are  119.8 179.3 25.23 P
nco signal index  44  from row number  18  in the original ncocx input file is not used.
Its coordn are  119.9 178.5 27.35 P
nco signal index  45  from row number  18  in the original ncocx input file is not used.
Its coordn are  119.9 178.5 23.9 P
nco signal index  48  from row number  19  in the original ncocx input file is not used.
Its coordn are  117.7 178.6 18.1 P
nco signal index  51  from row number  20  in the original ncocx input file is not used.
Its coordn are  121.2 176.1 22.35 P
nco signal index  52  from row number  21  in the original ncocx input file is not used.
Its coordn are  121.3 178.6 59.3 P
nco signal index  53  from row number  21  in the original ncocx input file is not used.
Its coordn are  121.3 178.6 30.0 P
nco signal index  54  from row number  21  in the original ncocx input file is not used.
Its coordn are  121.3 178.6 27.58 P
nco signal index  57  from row number  22  in the original ncocx input file is not used.
Its coordn are  122.2 178.3 26.64 P
nco signal index  64  from row number  25  in the original ncocx input file is not used.
Its coordn are  121.6 176.1 17.85 P
nco signal index  67  from row number  26  in the original ncocx input file is not used.
Its coordn are  118.9 179.3 22.85 P
nco signal index  68  from row number  26  in the original ncocx input file is not used.
Its coordn are  118.9 179.3 21.18 P
nco signal index  71  from row number  27  in the original ncocx input file is not used.
Its coordn are  107.9 177.9 27.83 P
nco signal index  74  from row number  28  in the original ncocx input file is not used.
Its coordn are  119.8 176.4 22.0 P
nco signal index  77  from row number  29  in the original ncocx input file is not used.
Its coordn are  107.7 178.0 24.1 P
nco signal index  78  from row number  29  in the original ncocx input file is not used.
Its coordn are  107.7 178.0 25.25 P
nco signal index  83  from row number  31  in the original ncocx input file is not used.
Its coordn are  113.1 176.0 25.1 P
nco signal index  84  from row number  31  in the original ncocx input file is not used.
Its coordn are  113.1 176.0 23.8 P
nco signal index  87  from row number  32  in the original ncocx input file is not used.
Its coordn are  113.8 176.6 30.35 P
nco signal index  93  from row number  34  in the original ncocx input file is not used.
Its coordn are  119.2 178.8 51.2 P
nco signal index  96  from row number  35  in the original ncocx input file is not used.
Its coordn are  118.5 176.6 25.42 P
nco signal index  99  from row number  36  in the original ncocx input file is not used.
Its coordn are  118.3 176.7 24.63 P
nco signal index  106  from row number  39  in the original ncocx input file is not used.
Its coordn are  120.9 179.5 34.65 P
nco signal index  109  from row number  40  in the original ncocx input file is not used.
Its coordn are  118.9 179.3 23.5 P
nco signal index  110  from row number  40  in the original ncocx input file is not used.
Its coordn are  118.9 179.3 21.4 P
nco signal index  113  from row number  41  in the original ncocx input file is not used.
Its coordn are  119.8 179.2 34.82 P
nco signal index  119  from row number  43  in the original ncocx input file is not used.
Its coordn are  114.2 178.0 21.85 P
nco signal index  120  from row number  43  in the original ncocx input file is not used.
Its coordn are  114.2 178.0 23.7 P
nco signal index  123  from row number  44  in the original ncocx input file is not used.
Its coordn are  112.6 174.7 31.82 P
nco signal index  129  from row number  47  in the original ncocx input file is not used.
Its coordn are  125.2 176.2 32.78 P
nco signal index  130  from row number  47  in the original ncocx input file is not used.
Its coordn are  125.2 176.2 27.95 P
nco signal index  133  from row number  48  in the original ncocx input file is not used.
Its coordn are  112.8 174.4 28.95 P
nco signal index  134  from row number  48  in the original ncocx input file is not used.
Its coordn are  112.8 174.4 27.12 P
nco signal index  135  from row number  48  in the original ncocx input file is not used.
Its coordn are  112.8 174.4 24.58 P
nco signal index  138  from row number  49  in the original ncocx input file is not used.
Its coordn are  137.2 174.9 28.56 P
nco signal index  139  from row number  49  in the original ncocx input file is not used.
Its coordn are  137.2 174.9 26.68 P
nco signal index  140  from row number  49  in the original ncocx input file is not used.
Its coordn are  137.2 174.9 23.58 P
nco signal index  141  from row number  50  in the original ncocx input file is not used.
Its coordn are  116.0 178.2 66.85 P
nco signal index  147  from row number  53  in the original ncocx input file is not used.
Its coordn are  112.2 176.7 22.51 P
nco signal index  148  from row number  53  in the original ncocx input file is not used.
Its coordn are  112.2 176.7 21.95 P
nco signal index  151  from row number  54  in the original ncocx input file is not used.
Its coordn are  118.3 176.7 23.42 P
nco signal index  157  from row number  56  in the original ncocx input file is not used.
Its coordn are  114.6 177.9 23.52 P
nco signal index  158  from row number  56  in the original ncocx input file is not used.
Its coordn are  114.6 177.9 21.65 P
nco signal index  164  from row number  58  in the original ncocx input file is not used.
Its coordn are  115.7 178.9 30.68 P
nco signal index  165  from row number  58  in the original ncocx input file is not used.
Its coordn are  115.7 178.9 43.1 P
nco signal index  168  from row number  59  in the original ncocx input file is not used.
Its coordn are  109.2 177.7 22.85 P
nco signal index  169  from row number  59  in the original ncocx input file is not used.
Its coordn are  109.2 177.7 22.03 P
nco signal index  172  from row number  60  in the original ncocx input file is not used.
Its coordn are  118.8 174.8 26.25 P
nco signal index  173  from row number  60  in the original ncocx input file is not used.
Its coordn are  118.8 174.8 18.05 P
nco signal index  174  from row number  60  in the original ncocx input file is not used.
Its coordn are  118.8 174.8 14.32 P
nco signal index  177  from row number  61  in the original ncocx input file is not used.
Its coordn are  103.2 177.1 25.85 P
nco signal index  178  from row number  61  in the original ncocx input file is not used.
Its coordn are  103.2 177.1 23.12 P
nco signal index  181  from row number  63  in the original ncocx input file is not used.
Its coordn are  119.2 179.2 31.41 P
nco signal index  182  from row number  63  in the original ncocx input file is not used.
Its coordn are  119.2 179.2 49.85 P
nco signal index  187  from row number  65  in the original ncocx input file is not used.
Its coordn are  119.1 177.2 49.25 P
nco signal index  190  from row number  66  in the original ncocx input file is not used.
Its coordn are  122.7 176.7 131.65 P
nco signal index  195  from row number  68  in the original ncocx input file is not used.
Its coordn are  121.5 176.3 26.68 P
nco signal index  196  from row number  68  in the original ncocx input file is not used.
Its coordn are  121.5 176.3 23.95 P
nco signal index  199  from row number  69  in the original ncocx input file is not used.
Its coordn are  120.8 177.1 109.35 P
nco signal index  202  from row number  70  in the original ncocx input file is not used.
Its coordn are  119.7 179.8 27.45 P
nco signal index  205  from row number  71  in the original ncocx input file is not used.
Its coordn are  122.3 178.5 179.75 P
nco signal index  210  from row number  73  in the original ncocx input file is not used.
Its coordn are  103.5 177.5 138.18 P
nco signal index  213  from row number  75  in the original ncocx input file is not used.
Its coordn are  118.9 179.3 22.94 P
nco signal index  214  from row number  75  in the original ncocx input file is not used.
Its coordn are  118.9 179.3 21.32 P
nco signal index  220  from row number  77  in the original ncocx input file is not used.
Its coordn are  118.3 179.7 27.95 P
nco signal index  221  from row number  77  in the original ncocx input file is not used.
Its coordn are  118.3 179.7 23.65 P
nco signal index  222  from row number  77  in the original ncocx input file is not used.
Its coordn are  118.3 179.7 21.87 P
nco signal index  227  from row number  79  in the original ncocx input file is not used.
Its coordn are  125.2 177.1 18.1 P
nco signal index  230  from row number  80  in the original ncocx input file is not used.
Its coordn are  118.7 177.3 22.25 P
nco signal index  231  from row number  80  in the original ncocx input file is not used.
Its coordn are  118.7 177.3 21.68 P
nco signal index  235  from row number  81  in the original ncocx input file is not used.
Its coordn are  124.5 178.9 17.68 P
nco signal index  236  from row number  81  in the original ncocx input file is not used.
Its coordn are  124.5 178.9 12.03 P
nco signal index  245  from row number  85  in the original ncocx input file is not used.
Its coordn are  119.5 175.0 21.23 P
nco signal index  248  from row number  86  in the original ncocx input file is not used.
Its coordn are  116.5 175.7 27.68 P
nco signal index  249  from row number  87  in the original ncocx input file is not used.
Its coordn are  139.5 171.9 49.57 P
nco signal index  250  from row number  87  in the original ncocx input file is not used.
Its coordn are  139.5 171.9 180.53 P
nco signal index  255  from row number  89  in the original ncocx input file is not used.
Its coordn are  124.6 175.7 27.65 P
nco signal index  256  from row number  90  in the original ncocx input file is not used.
Its coordn are  131.6 172.8 56.8 P
nco signal index  272  from row number  100  in the original ncocx input file is not used.
Its coordn are  117.7 178.5 27.48 P
nco signal index  275  from row number  101  in the original ncocx input file is not used.
Its coordn are  113.6 172.8 19.52 P
nco signal index  278  from row number  102  in the original ncocx input file is not used.
Its coordn are  120.2 174.2 175.9 P
nco signal index  282  from row number  103  in the original ncocx input file is not used.
Its coordn are  115.0 177.1 25.28 P
nco signal index  283  from row number  103  in the original ncocx input file is not used.
Its coordn are  115.0 177.1 21.9 P
nco signal index  288  from row number  105  in the original ncocx input file is not used.
Its coordn are  113.2 177.8 29.51 P
nco signal index  289  from row number  105  in the original ncocx input file is not used.
Its coordn are  113.2 177.8 43.87 P
nco signal index  292  from row number  106  in the original ncocx input file is not used.
Its coordn are  108.0 175.2 26.58 P
nco signal index  293  from row number  106  in the original ncocx input file is not used.
Its coordn are  108.0 175.2 25.74 P
nco signal index  294  from row number  106  in the original ncocx input file is not used.
Its coordn are  108.0 175.2 21.87 P
nco signal index  297  from row number  107  in the original ncocx input file is not used.
Its coordn are  108.3 177.8 26.47 P
nco signal index  298  from row number  107  in the original ncocx input file is not used.
Its coordn are  108.3 177.8 30.12 P
nco signal index  302  from row number  109  in the original ncocx input file is not used.
Its coordn are  121.5 176.4 25.76 P
nco signal index  303  from row number  109  in the original ncocx input file is not used.
Its coordn are  121.5 176.4 25.13 P
nco signal index  304  from row number  109  in the original ncocx input file is not used.
Its coordn are  121.5 176.4 22.23 P
nco signal index  309  from row number  111  in the original ncocx input file is not used.
Its coordn are  112.1 176.9 179.72 P
nco signal index  315  from row number  114  in the original ncocx input file is not used.
Its coordn are  118.4 178.6 22.43 P
nco signal index  316  from row number  114  in the original ncocx input file is not used.
Its coordn are  118.4 178.6 20.87 P
nco signal index  318  from row number  116  in the original ncocx input file is not used.
Its coordn are  139.5 172.3 50.29 P
nco signal index  319  from row number  116  in the original ncocx input file is not used.
Its coordn are  139.5 172.3 178.52 P
nco signal index  324  from row number  118  in the original ncocx input file is not used.
Its coordn are  109.3 179.1 180.53 P
nco signal index  328  from row number  120  in the original ncocx input file is not used.
Its coordn are  118.6 177.2 34.58 P
nco signal index  335  from row number  123  in the original ncocx input file is not used.
Its coordn are  120.2 179.1 26.85 P
nco signal index  336  from row number  123  in the original ncocx input file is not used.
Its coordn are  120.2 179.1 22.18 P
nco signal index  339  from row number  124  in the original ncocx input file is not used.
Its coordn are  123.3 176.9 25.31 P
nco signal index  340  from row number  124  in the original ncocx input file is not used.
Its coordn are  123.3 176.9 24.03 P
nco signal index  341  from row number  125  in the original ncocx input file is not used.
Its coordn are  137.9 176.6 54.43 P
nco signal index  347  from row number  128  in the original ncocx input file is not used.
Its coordn are  117.8 176.2 33.58 P
nco signal index  350  from row number  129  in the original ncocx input file is not used.
Its coordn are  120.5 180.8 26.79 P
nco signal index  351  from row number  129  in the original ncocx input file is not used.
Its coordn are  120.5 180.8 25.67 P
nco signal index  352  from row number  129  in the original ncocx input file is not used.
Its coordn are  120.5 180.8 24.13 P
nco signal index  355  from row number  130  in the original ncocx input file is not used.
Its coordn are  122.5 178.1 23.51 P
nco signal index  356  from row number  130  in the original ncocx input file is not used.
Its coordn are  122.5 178.1 21.2 P
nco signal index  361  from row number  132  in the original ncocx input file is not used.
Its coordn are  117.6 178.0 30.56 P
nco signal index  362  from row number  132  in the original ncocx input file is not used.
Its coordn are  117.6 178.0 17.78 P
nco signal index  365  from row number  133  in the original ncocx input file is not used.
Its coordn are  124.7 177.1 21.87 P
nco signal index  374  from row number  137  in the original ncocx input file is not used.
Its coordn are  119.5 178.4 27.45 P
nco signal index  375  from row number  137  in the original ncocx input file is not used.
Its coordn are  119.5 178.4 26.64 P
nco signal index  376  from row number  137  in the original ncocx input file is not used.
Its coordn are  119.5 178.4 23.73 P
nco signal index  379  from row number  138  in the original ncocx input file is not used.
Its coordn are  126.4 176.1 32.85 P
nco signal index  384  from row number  140  in the original ncocx input file is not used.
Its coordn are  118.9 176.1 131.2 P
nco signal index  387  from row number  141  in the original ncocx input file is not used.
Its coordn are  117.3 177.2 25.34 P
nco signal index  388  from row number  141  in the original ncocx input file is not used.
Its coordn are  117.3 177.2 43.79 P
nco signal index  392  from row number  142  in the original ncocx input file is not used.
Its coordn are  121.9 176.3 182.75 P
nco signal index  395  from row number  143  in the original ncocx input file is not used.
Its coordn are  123.0 178.0 22.86 P
nco signal index  396  from row number  143  in the original ncocx input file is not used.
Its coordn are  123.0 178.0 21.24 P
nco signal index  401  from row number  145  in the original ncocx input file is not used.
Its coordn are  119.2 179.3 27.95 P
nco signal index  404  from row number  146  in the original ncocx input file is not used.
Its coordn are  123.3 177.1 27.03 P
nco signal index  405  from row number  146  in the original ncocx input file is not used.
Its coordn are  123.3 177.1 25.41 P
nco signal index  414  from row number  152  in the original ncocx input file is not used.
Its coordn are  119.5 179.2 31.4 P
nco signal index  415  from row number  152  in the original ncocx input file is not used.
Its coordn are  119.5 179.2 49.8 P
nco signal index  421  from row number  155  in the original ncocx input file is not used.
Its coordn are  121.2 176.6 181.25 P
nco signal index  424  from row number  156  in the original ncocx input file is not used.
Its coordn are  119.0 177.1 18.75 P
nco signal index  425  from row number  156  in the original ncocx input file is not used.
Its coordn are  119.0 177.1 14.73 P
nco signal index  431  from row number  158  in the original ncocx input file is not used.
Its coordn are  119.8 178.8 32.37 P
nco signal index  432  from row number  158  in the original ncocx input file is not used.
Its coordn are  119.8 178.8 176.74 P
nco signal index  436  from row number  160  in the original ncocx input file is not used.
Its coordn are  112.5 177.8 27.68 P
nco signal index  437  from row number  160  in the original ncocx input file is not used.
Its coordn are  112.5 177.8 51.03 P
nco signal index  442  from row number  162  in the original ncocx input file is not used.
Its coordn are  127.6 176.5 36.31 P
nco signal index  443  from row number  162  in the original ncocx input file is not used.
Its coordn are  127.6 176.5 184.45 P
nco signal index  447  from row number  164  in the original ncocx input file is not used.
Its coordn are  116.8 177.1 39.42 P
nco signal index  448  from row number  164  in the original ncocx input file is not used.
Its coordn are  116.8 177.1 138.18 P
nco signal index  451  from row number  165  in the original ncocx input file is not used.
Its coordn are  121.3 176.1 24.13 P
nco signal index  456  from row number  167  in the original ncocx input file is not used.
Its coordn are  121.9 175.5 138.17 P
nco signal index  461  from row number  169  in the original ncocx input file is not used.
Its coordn are  120.6 179.3 180.34 P
nco signal index  464  from row number  170  in the original ncocx input file is not used.
Its coordn are  122.2 177.8 27.38 P
nco signal index  465  from row number  170  in the original ncocx input file is not used.
Its coordn are  122.2 177.8 43.95 P
nco signal index  466  from row number  171  in the original ncocx input file is not used.
Its coordn are  119.3 178.3 57.14 P
nco signal index  467  from row number  171  in the original ncocx input file is not used.
Its coordn are  119.3 178.3 41.7 P
nco signal index  468  from row number  171  in the original ncocx input file is not used.
Its coordn are  119.3 178.3 27.42 P
nco signal index  469  from row number  171  in the original ncocx input file is not used.
Its coordn are  119.3 178.3 26.54 P
nco signal index  470  from row number  171  in the original ncocx input file is not used.
Its coordn are  119.3 178.3 23.78 P
nco signal index  474  from row number  172  in the original ncocx input file is not used.
Its coordn are  119.1 177.1 17.84 P
nco signal index  475  from row number  172  in the original ncocx input file is not used.
Its coordn are  119.1 177.1 14.93 P
nco signal index  478  from row number  173  in the original ncocx input file is not used.
Its coordn are  120.9 179.5 25.41 P
nco signal index  479  from row number  173  in the original ncocx input file is not used.
Its coordn are  120.9 179.5 30.68 P
nco signal index  484  from row number  175  in the original ncocx input file is not used.
Its coordn are  120.9 180.3 22.43 P
nco signal index  487  from row number  176  in the original ncocx input file is not used.
Its coordn are  103.1 177.5 34.43 P
nco signal index  493  from row number  179  in the original ncocx input file is not used.
Its coordn are  122.4 177.9 180.79 P
nco signal index  496  from row number  181  in the original ncocx input file is not used.
Its coordn are  135.9 175.9 30.75 P
nco signal index  497  from row number  181  in the original ncocx input file is not used.
Its coordn are  135.9 175.9 50.03 P
nco signal index  512  from row number  187  in the original ncocx input file is not used.
Its coordn are  117.5 179.3 49.38 P
nco signal index  515  from row number  188  in the original ncocx input file is not used.
Its coordn are  121.2 176.1 21.31 P
nco signal index  518  from row number  189  in the original ncocx input file is not used.
Its coordn are  117.3 176.8 18.93 P
nco signal index  519  from row number  189  in the original ncocx input file is not used.
Its coordn are  117.3 176.8 14.68 P
nco signal index  522  from row number  190  in the original ncocx input file is not used.
Its coordn are  120.9 180.2 24.56 P
nco signal index  523  from row number  190  in the original ncocx input file is not used.
Its coordn are  120.9 180.2 18.14 P
nco signal index  524  from row number  190  in the original ncocx input file is not used.
Its coordn are  120.9 180.2 13.2 P
nco signal index  533  from row number  194  in the original ncocx input file is not used.
Its coordn are  113.2 178.1 43.76 P
nco signal index  534  from row number  194  in the original ncocx input file is not used.
Its coordn are  113.2 178.1 152.78 P
nco signal index  537  from row number  195  in the original ncocx input file is not used.
Its coordn are  114.9 177.9 33.95 P
nco signal index  540  from row number  196  in the original ncocx input file is not used.
Its coordn are  113.1 177.4 27.68 P
nco signal index  548  from row number  199  in the original ncocx input file is not used.
Its coordn are  115.7 178.2 49.85 P
nco signal index  551  from row number  200  in the original ncocx input file is not used.
Its coordn are  123.4 178.6 174.38 P
nco signal index  554  from row number  201  in the original ncocx input file is not used.
Its coordn are  119.5 178.4 27.93 P
nco signal index  555  from row number  201  in the original ncocx input file is not used.
Its coordn are  119.5 178.4 18.46 P
nco signal index  558  from row number  202  in the original ncocx input file is not used.
Its coordn are  115.7 177.5 34.62 P
nco signal index  559  from row number  202  in the original ncocx input file is not used.
Its coordn are  115.7 177.5 182.47 P
nco signal index  568  from row number  205  in the original ncocx input file is not used.
Its coordn are  119.5 177.2 17.85 P
nco signal index  569  from row number  205  in the original ncocx input file is not used.
Its coordn are  119.5 177.2 14.67 P
nco signal index  581  from row number  211  in the original ncocx input file is not used.
Its coordn are  124.7 175.5 22.35 P
nco signal index  584  from row number  212  in the original ncocx input file is not used.
Its coordn are  111.7 174.4 27.14 P
nco signal index  585  from row number  212  in the original ncocx input file is not used.
Its coordn are  111.7 174.4 24.68 P
nco signal index  588  from row number  213  in the original ncocx input file is not used.
Its coordn are  110.1 174.2 22.03 P
nco signal index  591  from row number  214  in the original ncocx input file is not used.
Its coordn are  131.8 173.2 22.15 P
nco signal index  593  from row number  215  in the original ncocx input file is not used.
Its coordn are  103.3 178.4 49.5 P
nco signal index  600  from row number  219  in the original ncocx input file is not used.
Its coordn are  117.2 176.3 18.85 P
nco signal index  601  from row number  219  in the original ncocx input file is not used.
Its coordn are  117.2 176.3 14.93 P
nco signal index  604  from row number  220  in the original ncocx input file is not used.
Its coordn are  119.2 179.0 24.98 P
nco signal index  607  from row number  221  in the original ncocx input file is not used.
Its coordn are  118.9 176.1 130.99 P
nco signal index  611  from row number  223  in the original ncocx input file is not used.
Its coordn are  119.9 178.5 26.79 P
nco signal index  612  from row number  223  in the original ncocx input file is not used.
Its coordn are  119.9 178.5 25.18 P
nco signal index  613  from row number  223  in the original ncocx input file is not used.
Its coordn are  119.9 178.5 22.23 P
nco signal index  615  from row number  224  in the original ncocx input file is not used.
Its coordn are  118.4 179.5 40.56 P
nco signal index  618  from row number  225  in the original ncocx input file is not used.
Its coordn are  118.2 178.4 27.03 P
nco signal index  620  from row number  226  in the original ncocx input file is not used.
Its coordn are  119.3 178.9 35.87 P
nco signal index  621  from row number  226  in the original ncocx input file is not used.
Its coordn are  119.3 178.9 182.78 P
################################################################
The following list the nco signals used more than their given degeneracy values (overused) in match finding:
nco signal index  12  from row number  4  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  128.6 175.7 61.0 P
nco signal index  21  from row number  8  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  134.5 171.3 44.16 P
nco signal index  22  from row number  9  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  122.8 177.1 64.5 P
nco signal index  23  from row number  10  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.1 174.9 51.9 P
nco signal index  24  from row number  10  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.1 174.9 19.62 P
nco signal index  37  from row number  16  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.7 176.8 64.51 P
nco signal index  38  from row number  17  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.8 179.3 60.0 P
nco signal index  41  from row number  17  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.8 179.3 27.25 P
nco signal index  46  from row number  19  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  117.7 178.6 64.9 P
nco signal index  49  from row number  20  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  19  times in match finding.
Its coordn are  121.2 176.1 67.0 P
nco signal index  50  from row number  20  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  121.2 176.1 68.3 P
nco signal index  58  from row number  23  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.5 180.9 54.83 P
nco signal index  59  from row number  23  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.5 180.9 17.9 P
nco signal index  62  from row number  25  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.6 176.1 67.07 P
nco signal index  63  from row number  25  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.6 176.1 68.27 P
nco signal index  65  from row number  26  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  14  times in match finding.
Its coordn are  118.9 179.3 66.83 P
nco signal index  66  from row number  26  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  18  times in match finding.
Its coordn are  118.9 179.3 31.77 P
nco signal index  79  from row number  30  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  120.0 173.9 44.4 P
nco signal index  80  from row number  31  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  113.1 176.0 55.63 P
nco signal index  88  from row number  33  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  140.3 173.9 55.32 P
nco signal index  89  from row number  33  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  140.3 173.9 64.36 P
nco signal index  90  from row number  34  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  119.2 178.8 64.86 P
nco signal index  91  from row number  34  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.2 178.8 32.0 P
nco signal index  97  from row number  36  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  118.3 176.7 66.01 P
nco signal index  98  from row number  36  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.3 176.7 68.3 P
nco signal index  100  from row number  37  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  120.3 177.6 57.74 P
nco signal index  101  from row number  37  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.3 177.6 32.25 P
nco signal index  102  from row number  37  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.3 177.6 31.58 P
nco signal index  103  from row number  38  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.8 180.9 54.83 P
nco signal index  104  from row number  38  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.8 180.9 17.8 P
nco signal index  105  from row number  39  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.9 179.5 60.0 P
nco signal index  107  from row number  40  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  12  times in match finding.
Its coordn are  118.9 179.3 66.82 P
nco signal index  108  from row number  40  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  18  times in match finding.
Its coordn are  118.9 179.3 31.94 P
nco signal index  111  from row number  41  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.8 179.2 60.47 P
nco signal index  112  from row number  41  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.8 179.2 29.99 P
nco signal index  114  from row number  42  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  120.0 180.9 54.84 P
nco signal index  115  from row number  42  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  120.0 180.9 17.9 P
nco signal index  116  from row number  43  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  114.2 178.0 58.26 P
nco signal index  124  from row number  45  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  118.9 174.9 60.4 P
nco signal index  125  from row number  45  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  118.9 174.9 63.7 P
nco signal index  126  from row number  46  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  140.2 173.9 55.5 P
nco signal index  127  from row number  46  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  140.2 173.9 64.36 P
nco signal index  128  from row number  47  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  125.2 176.2 64.58 P
nco signal index  132  from row number  48  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  112.8 174.4 45.0 P
nco signal index  145  from row number  53  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  112.2 176.7 65.88 P
nco signal index  146  from row number  53  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  112.2 176.7 32.14 P
nco signal index  149  from row number  54  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  118.3 176.7 66.0 P
nco signal index  150  from row number  54  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.3 176.7 68.1 P
nco signal index  154  from row number  56  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  114.6 177.9 58.3 P
nco signal index  159  from row number  57  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  118.5 177.3 56.6 P
nco signal index  160  from row number  57  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  118.5 177.3 30.88 P
nco signal index  161  from row number  57  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  118.5 177.3 32.58 P
nco signal index  166  from row number  59  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  109.2 177.7 65.52 P
nco signal index  167  from row number  59  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  109.2 177.7 32.05 P
nco signal index  170  from row number  60  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  118.8 174.8 63.62 P
nco signal index  171  from row number  60  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  118.8 174.8 38.9 P
nco signal index  179  from row number  62  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  134.8 171.3 44.12 P
nco signal index  180  from row number  63  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  119.2 179.2 64.8 P
nco signal index  183  from row number  64  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  131.9 176.0 56.99 P
nco signal index  184  from row number  64  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  131.9 176.0 15.44 P
nco signal index  185  from row number  65  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  13  times in match finding.
Its coordn are  119.1 177.2 65.97 P
nco signal index  186  from row number  65  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  119.1 177.2 31.5 P
nco signal index  191  from row number  67  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  118.0 177.7 54.92 P
nco signal index  192  from row number  67  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  118.0 177.7 18.24 P
nco signal index  197  from row number  69  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.8 177.1 57.11 P
nco signal index  198  from row number  69  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.8 177.1 28.12 P
nco signal index  200  from row number  70  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.7 179.8 58.2 P
nco signal index  201  from row number  70  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.7 179.8 31.4 P
nco signal index  203  from row number  71  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  122.3 178.5 57.4 P
nco signal index  204  from row number  71  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  122.3 178.5 40.8 P
nco signal index  206  from row number  72  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  123.3 178.4 54.7 P
nco signal index  207  from row number  72  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  123.3 178.4 18.0 P
nco signal index  211  from row number  74  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  122.1 176.1 47.71 P
nco signal index  212  from row number  75  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  10  times in match finding.
Its coordn are  118.9 179.3 66.8 P
nco signal index  215  from row number  76  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.0 179.5 60.47 P
nco signal index  223  from row number  78  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.9 179.1 59.24 P
nco signal index  224  from row number  78  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.9 179.1 28.07 P
nco signal index  225  from row number  79  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  125.2 177.1 66.4 P
nco signal index  226  from row number  79  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  125.2 177.1 68.6 P
nco signal index  228  from row number  80  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  118.7 177.3 66.1 P
nco signal index  229  from row number  80  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  118.7 177.3 30.9 P
nco signal index  232  from row number  81  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  124.5 178.9 63.24 P
nco signal index  237  from row number  82  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  122.7 180.5 55.0 P
nco signal index  238  from row number  82  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  122.7 180.5 17.78 P
nco signal index  239  from row number  83  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  121.1 180.5 54.86 P
nco signal index  240  from row number  83  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  121.1 180.5 18.37 P
nco signal index  246  from row number  86  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.5 175.7 57.54 P
nco signal index  247  from row number  86  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  116.5 175.7 31.08 P
nco signal index  251  from row number  88  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  115.3 178.1 64.4 P
nco signal index  253  from row number  89  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  124.6 175.7 55.64 P
nco signal index  254  from row number  89  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  124.6 175.7 29.44 P
nco signal index  261  from row number  94  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  117.9 173.8 44.8 P
nco signal index  262  from row number  95  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  108.6 177.8 56.37 P
nco signal index  263  from row number  95  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  108.6 177.8 29.78 P
nco signal index  264  from row number  96  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.9 173.8 44.3 P
nco signal index  265  from row number  97  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  112.4 176.7 57.54 P
nco signal index  266  from row number  97  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  112.4 176.7 31.08 P
nco signal index  267  from row number  98  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.7 174.7 44.7 P
nco signal index  268  from row number  99  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.3 177.3 57.11 P
nco signal index  269  from row number  99  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.3 177.3 28.07 P
nco signal index  273  from row number  101  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  113.6 172.8 63.0 P
nco signal index  274  from row number  101  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  113.6 172.8 66.3 P
nco signal index  279  from row number  103  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  115.0 177.1 58.3 P
nco signal index  280  from row number  103  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  115.0 177.1 42.4 P
nco signal index  284  from row number  104  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.7 178.5 56.1 P
nco signal index  307  from row number  111  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  112.1 176.9 56.8 P
nco signal index  308  from row number  111  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  112.1 176.9 40.7 P
nco signal index  310  from row number  112  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  113.0 174.6 44.9 P
nco signal index  313  from row number  114  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  118.4 178.6 64.9 P
nco signal index  320  from row number  117  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  115.7 177.5 64.42 P
nco signal index  321  from row number  118  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  109.3 179.1 60.13 P
nco signal index  325  from row number  119  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.5 175.8 47.08 P
nco signal index  326  from row number  120  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  10  times in match finding.
Its coordn are  118.6 177.2 59.94 P
nco signal index  327  from row number  120  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  118.6 177.2 28.76 P
nco signal index  329  from row number  121  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  117.1 180.0 54.6 P
nco signal index  330  from row number  121  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  117.1 180.0 18.38 P
nco signal index  342  from row number  126  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  101.9 179.5 66.62 P
nco signal index  343  from row number  126  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  101.9 179.5 32.03 P
nco signal index  345  from row number  128  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  117.8 176.2 60.52 P
nco signal index  346  from row number  128  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  117.8 176.2 29.14 P
nco signal index  353  from row number  130  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  122.5 178.1 67.24 P
nco signal index  354  from row number  130  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  122.5 178.1 32.07 P
nco signal index  357  from row number  131  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 181.8 54.92 P
nco signal index  358  from row number  131  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 181.8 18.99 P
nco signal index  363  from row number  133  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  10  times in match finding.
Its coordn are  124.7 177.1 66.3 P
nco signal index  364  from row number  133  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  124.7 177.1 68.46 P
nco signal index  368  from row number  135  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  125.9 176.2 62.8 P
nco signal index  369  from row number  135  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  125.9 176.2 63.3 P
nco signal index  372  from row number  137  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.5 178.4 58.14 P
nco signal index  373  from row number  137  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.5 178.4 41.7 P
nco signal index  382  from row number  140  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  118.9 176.1 63.2 P
nco signal index  383  from row number  140  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.9 176.1 39.0 P
nco signal index  385  from row number  141  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  117.3 177.2 60.58 P
nco signal index  386  from row number  141  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  117.3 177.2 29.86 P
nco signal index  389  from row number  142  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.9 176.3 59.6 P
nco signal index  393  from row number  143  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  123.0 178.0 67.2 P
nco signal index  394  from row number  143  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  123.0 178.0 32.12 P
nco signal index  397  from row number  144  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  113.2 177.1 54.9 P
nco signal index  398  from row number  144  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  113.2 177.1 17.4 P
nco signal index  402  from row number  146  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 177.1 56.4 P
nco signal index  403  from row number  146  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 177.1 43.34 P
nco signal index  406  from row number  147  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  120.7 176.1 52.0 P
nco signal index  407  from row number  147  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  120.7 176.1 19.7 P
nco signal index  412  from row number  151  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  134.5 171.4 44.16 P
nco signal index  413  from row number  152  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.5 179.2 64.8 P
nco signal index  419  from row number  155  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  121.2 176.6 54.6 P
nco signal index  420  from row number  155  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  121.2 176.6 41.2 P
nco signal index  422  from row number  156  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  14  times in match finding.
Its coordn are  119.0 177.1 66.1 P
nco signal index  423  from row number  156  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  13  times in match finding.
Its coordn are  119.0 177.1 38.1 P
nco signal index  426  from row number  157  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  126.7 173.7 60.7 P
nco signal index  427  from row number  157  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  126.7 173.7 29.17 P
nco signal index  434  from row number  160  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  112.5 177.8 64.93 P
nco signal index  440  from row number  162  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  127.6 176.5 54.94 P
nco signal index  441  from row number  162  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  127.6 176.5 32.21 P
nco signal index  445  from row number  163  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  124.2 175.1 64.16 P
nco signal index  449  from row number  165  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  18  times in match finding.
Its coordn are  121.3 176.1 67.09 P
nco signal index  450  from row number  165  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  24  times in match finding.
Its coordn are  121.3 176.1 31.8 P
nco signal index  452  from row number  166  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 179.1 58.26 P
nco signal index  453  from row number  166  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.3 179.1 39.91 P
nco signal index  457  from row number  168  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  115.3 177.8 54.61 P
nco signal index  458  from row number  168  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  115.3 177.8 18.5 P
nco signal index  471  from row number  172  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  12  times in match finding.
Its coordn are  119.1 177.1 66.04 P
nco signal index  472  from row number  172  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  17  times in match finding.
Its coordn are  119.1 177.1 38.13 P
nco signal index  473  from row number  172  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.1 177.1 30.12 P
nco signal index  476  from row number  173  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.9 179.5 60.0 P
nco signal index  477  from row number  173  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  120.9 179.5 32.95 P
nco signal index  480  from row number  174  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  117.5 177.2 54.5 P
nco signal index  481  from row number  174  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  117.5 177.2 18.5 P
nco signal index  482  from row number  175  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.9 180.3 67.32 P
nco signal index  483  from row number  175  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  120.9 180.3 31.63 P
nco signal index  485  from row number  176  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  103.1 177.5 59.95 P
nco signal index  486  from row number  176  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  103.1 177.5 29.06 P
nco signal index  488  from row number  177  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  117.9 173.8 44.94 P
nco signal index  489  from row number  178  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  117.2 173.5 59.16 P
nco signal index  490  from row number  178  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  117.2 173.5 65.95 P
nco signal index  491  from row number  179  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  122.4 177.9 54.8 P
nco signal index  492  from row number  179  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  122.4 177.9 40.8 P
nco signal index  495  from row number  181  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  135.9 175.9 61.3 P
nco signal index  498  from row number  182  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  110.2 179.1 66.4 P
nco signal index  499  from row number  182  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  110.2 179.1 32.27 P
nco signal index  503  from row number  183  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  122.2 174.7 62.59 P
nco signal index  504  from row number  184  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  115.7 177.7 52.09 P
nco signal index  505  from row number  184  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  115.7 177.7 20.07 P
nco signal index  506  from row number  185  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  119.1 176.4 61.0 P
nco signal index  509  from row number  186  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  131.9 176.0 56.99 P
nco signal index  510  from row number  186  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  131.9 176.0 15.44 P
nco signal index  511  from row number  187  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  117.5 179.3 65.96 P
nco signal index  513  from row number  188  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  18  times in match finding.
Its coordn are  121.2 176.1 67.09 P
nco signal index  514  from row number  188  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  24  times in match finding.
Its coordn are  121.2 176.1 31.8 P
nco signal index  516  from row number  189  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  117.3 176.8 66.4 P
nco signal index  517  from row number  189  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  117.3 176.8 37.9 P
nco signal index  520  from row number  190  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  120.9 180.2 66.8 P
nco signal index  530  from row number  194  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  113.2 178.1 60.05 P
nco signal index  532  from row number  194  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  113.2 178.1 28.85 P
nco signal index  542  from row number  197  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  121.0 177.2 64.95 P
nco signal index  543  from row number  198  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  136.9 175.5 55.82 P
nco signal index  546  from row number  199  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  115.7 178.2 66.85 P
nco signal index  547  from row number  199  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  115.7 178.2 32.28 P
nco signal index  549  from row number  200  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.4 178.6 57.4 P
nco signal index  550  from row number  200  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  123.4 178.6 39.31 P
nco signal index  556  from row number  202  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  115.7 177.5 60.6 P
nco signal index  557  from row number  202  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  115.7 177.5 28.79 P
nco signal index  560  from row number  203  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.7 178.5 60.6 P
nco signal index  561  from row number  203  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.7 178.5 27.7 P
nco signal index  565  from row number  205  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  7  times in match finding.
Its coordn are  119.5 177.2 65.97 P
nco signal index  566  from row number  205  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.5 177.2 38.13 P
nco signal index  570  from row number  206  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  114.2 177.4 60.45 P
nco signal index  571  from row number  206  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  114.2 177.4 31.18 P
nco signal index  572  from row number  206  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  114.2 177.4 28.78 P
nco signal index  573  from row number  207  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  10  times in match finding.
Its coordn are  124.7 177.0 66.3 P
nco signal index  574  from row number  207  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  8  times in match finding.
Its coordn are  124.7 177.0 68.3 P
nco signal index  577  from row number  210  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  116.9 173.4 59.1 P
nco signal index  578  from row number  210  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  116.9 173.4 65.8 P
nco signal index  583  from row number  212  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  111.7 174.4 44.7 P
nco signal index  586  from row number  213  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  110.1 174.2 62.69 P
nco signal index  592  from row number  215  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  103.3 178.4 65.9 P
nco signal index  594  from row number  216  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.7 175.9 47.1 P
nco signal index  595  from row number  217  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  120.9 179.5 60.0 P
nco signal index  598  from row number  219  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  117.2 176.3 66.43 P
nco signal index  599  from row number  219  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  117.2 176.3 37.9 P
nco signal index  602  from row number  220  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  119.2 179.0 59.4 P
nco signal index  603  from row number  220  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  6  times in match finding.
Its coordn are  119.2 179.0 32.7 P
nco signal index  605  from row number  221  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  5  times in match finding.
Its coordn are  118.9 176.1 63.15 P
nco signal index  606  from row number  221  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  118.9 176.1 39.06 P
nco signal index  608  from row number  222  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  9  times in match finding.
Its coordn are  119.2 177.2 65.97 P
nco signal index  619  from row number  226  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  4  times in match finding.
Its coordn are  119.3 178.9 59.3 P
nco signal index  622  from row number  227  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  114.4 176.1 57.76 P
nco signal index  623  from row number  227  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  114.4 176.1 31.21 P
nco signal index  624  from row number  228  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  2  times in match finding.
Its coordn are  140.6 173.9 55.35 P
nco signal index  625  from row number  228  in the original ncocx input file is overused.
Its degeneracy value is  1 . It was used  3  times in match finding.
Its coordn are  140.6 173.9 64.4 P
In summary, the nco signal usage for matching nca asgn is described below:
there are  170  nco signals used for matching nca asgn within their specified degeneracy range.
there are  211  nco signals are never used to match any nca asgn.
there are  230  nco signals are used over their allowed degeneracy number to match nca asgns.
