	
Operating parameters
	Forest species (N)*

	
	X1=Fagus sylvatica
	X2=Quercus petraea
	X3=Pinus brutia

	Y1=Normal conditions
	XY1.1 (12)*
	XY2.2 (12)
	XY3.1 (12)

	Y2=Improper maintenance
	XY1.2 (12)
	XY2.2 (12)
	XY3.2 (12)

	Y3=Infrequent accelerator
	XY1.3 (12)
	XY2.3 (12)
	XY3.3 (12)


Table 1 Measurement conditions of wood dust produced by different forest species and operating parameters





*(N): number of samples

