Table 3 Main characteristics of the sampling sites. Fagus sylvatica (Fs.), Quercus sp. (Q.), Pinus brutia (Pbr.)

	Operating parameters
	Forest 
species
	
	Tree 
processed (n)
	Average
DBH (cm)
	Number of 
samples (Ν)

	
Normal conditions
	Fs.
	XY1.1
	45
	60.48
	12

	
	Q.
	XY2.1
	91
	38.57
	12

	
	Pbr.
	XY3.1
	256
	30.78
	12

	
Improper maintenance
	Fs.
	XY1.2
	33
	75.33
	12

	
	Q.
	XY2.2
	86
	37.27
	12

	
	Pbr.
	XY3.2
	213
	31.44
	12

	
Infrequent accelerator
	Fs.
	XY1.3
	40
	60.75
	12

	
	Q.
	XY2.3
	88
	39.34
	12

	
	Pbr.
	XY3.3
	217
	31.87
	12





