We studied the transport process and deposition law of dust particles under the action of wind: when the wind field is the same, the transport process can be divided into a raising section and a settling section, and the raising wind has a sorting effect on the height of different particle sizes. The ideal transport distance of particles corresponding to different raising wind is inversely proportional to the square of their particle size.
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