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Appendix I

Appendix I presents the geometry of under-study structure, giving details for concrete and steel members. 
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Figure 25: Concrete members of structure, elevations +5.75m, +10.025m, +16.025m & +20.57m
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Figure 26: Details of reinforcement for concrete columns C1, C2, concrete beams B1, B2, B3 and concrete slab d=1200mm
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[bookmark: _Hlk148902702]Figure 27: Detail presentation of steel sections for alignments 1 & 2
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Figure 28: Detail presentation of steel sections for alignments A & B



Figure 29: (left) Detail of base plate-connection between concrete and steel members of structure, (right) detail of guides





















Appendix II

Table 7. Number of modes, modal mass participation and cumulative modal mass participation
	No Mode
	Period
	Mass Participation UX
	Mass Participation UY
	Mass Participation RZ
	SumUX
	SumUY
	SumRZ

	
	Sec
	%
	%
	%
	%
	%
	%

	1
	0,957219
	0,967
	67,919
	0,196
	0,967
	67,919
	0,196

	2
	0,945865
	69,854
	0,996
	0,21
	70,82
	68,915
	0,406

	3
	0,562138
	2,871
	0,488
	67,064
	73,691
	69,402
	67,47

	4
	0,548923
	0,033
	15,169
	0,488
	73,724
	84,571
	67,958

	5
	0,502866
	11,927
	0,004982
	8,421
	85,651
	84,576
	76,379

	6
	0,415466
	0,001434
	0,005122
	0,000187
	85,652
	84,582
	76,379

	7
	0,354485
	0,000161
	1,434
	0,044
	85,653
	86,016
	76,423

	8
	0,313689
	0,008231
	5,3E-06
	0,005944
	85,661
	86,016
	76,429

	9
	0,300984
	7,59E-06
	0,024
	4,53E-05
	85,661
	86,04
	76,429

	10
	0,288807
	0,000752
	0,005456
	0,001806
	85,662
	86,045
	76,431

	11
	0,283306
	0,000138
	2,1E-05
	7,528
	85,662
	86,045
	83,959

	12
	0,265434
	0,00124
	0,006798
	0,001207
	85,663
	86,052
	83,96

	13
	0,253271
	0,155
	0,00052
	1,83E-05
	85,818
	86,052
	83,96

	14
	0,225109
	0,131
	0,002107
	0,000436
	85,949
	86,055
	83,961

	15
	0,217151
	0,15
	3,43E-05
	0,004178
	86,099
	86,055
	83,965

	16
	0,213064
	0,755
	1,36E-05
	0,012
	86,854
	86,055
	83,977

	17
	0,207652
	0,346
	0,089
	4,45E-08
	87,2
	86,143
	83,977

	18
	0,206271
	0,145
	0,186
	0,008381
	87,345
	86,329
	83,985

	19
	0,20189
	0,001598
	0,001852
	7,22E-06
	87,347
	86,331
	83,985

	20
	0,198655
	1,2E-06
	6,44E-06
	5,63E-09
	87,347
	86,331
	83,985

	21
	0,19782
	0,000557
	0,016
	1,71E-06
	87,347
	86,347
	83,985

	22
	0,190019
	5,63E-06
	5,03E-06
	6,44E-06
	87,347
	86,347
	83,985

	23
	0,186339
	3,02E-05
	0,005371
	1,33E-05
	87,347
	86,352
	83,985

	24
	0,185891
	5,09E-07
	0,000187
	6,49E-07
	87,347
	86,353
	83,985

	25
	0,174565
	0,00033
	0,000127
	1,02E-06
	87,348
	86,353
	83,985

	26
	0,172806
	0,000853
	0,09
	0,000526
	87,349
	86,443
	83,986

	27
	0,168884
	0,091
	3,874
	0,034
	87,44
	90,317
	84,02

	28
	0,168488
	0,016
	1,211
	0,00187
	87,456
	91,528
	84,022

	29
	0,167333
	0,001007
	0,001862
	5,2E-05
	87,457
	91,53
	84,022

	30
	0,163062
	1,9E-06
	6,91E-05
	9,83E-08
	87,457
	91,53
	84,022

	31
	0,162084
	0,065
	0,012
	0,003067
	87,522
	91,542
	84,025

	32
	0,160661
	4,456
	0,165
	0,265
	91,977
	91,707
	84,29

	33
	0,159441
	0,00201
	7,86E-05
	5,1E-05
	91,979
	91,707
	84,29

	34
	0,157816
	0,009607
	0,213
	0,004112
	91,989
	91,92
	84,294

	35
	0,157376
	0,009214
	0,00153
	0,000486
	91,998
	91,921
	84,295

	36
	0,156613
	0,105
	0,465
	0,0002
	92,103
	92,387
	84,295

	37
	0,153689
	0,051
	0,007271
	0,006277
	92,154
	92,394
	84,301

	38
	0,151225
	1,43E-05
	0,004332
	0,000381
	92,154
	92,398
	84,301

	39
	0,150492
	1,756
	0,596
	0,464
	93,91
	92,994
	84,765

	40
	0,147319
	0,142
	0,374
	0,105
	94,052
	93,367
	84,871

	41
	0,145611
	2,82E-05
	0,000135
	2,86E-05
	94,052
	93,368
	84,871

	42
	0,14298
	0,023
	0,374
	0,031
	94,075
	93,741
	84,901

	43
	0,142643
	0,017
	0,394
	0,026
	94,092
	94,135
	84,927

	44
	0,136334
	0,00921
	0,022
	1,03E-05
	94,102
	94,157
	84,927

	45
	0,135456
	9,98E-05
	0,000135
	2,79E-07
	94,102
	94,158
	84,927

	46
	0,133697
	0,09
	0,003162
	0,156
	94,192
	94,161
	85,084

	47
	0,132063
	9,74E-12
	2,43E-10
	1,17E-09
	94,192
	94,161
	85,084

	48
	0,132061
	1,86E-11
	8,62E-10
	2,83E-12
	94,192
	94,161
	85,084

	49
	0,130424
	0,002651
	0,000886
	0,553
	94,194
	94,162
	85,637

	50
	0,128353
	0,00057
	0,008942
	0,24
	94,195
	94,171
	85,877

	51
	0,1276
	0,000752
	0,015
	0,000172
	94,196
	94,185
	85,877

	52
	0,126119
	0,01
	0,001999
	5,254
	94,206
	94,187
	91,131
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