

Highlights
· Low temperature physical method was applied priority to separating hazardous As2O3.
· Flexible separation and purification of vaporization and condensation was established.
· Sb2O3 products were prepared directly from Hazardous waste arsenic antimony dust.

