
Table 5. Correspondent BoAM list of the armored FLDS considering the DfA2 method. 
	Nb.
	FLDS armored parts Image
	Armored part name 
	Ballistic  protected material
	Dimensions
(mm)
	Estimat.
mass (kg)
	Attach. type

	1
	[image: ]
	Side impact bar cover
	Aramid fiber 9 layers
	863 x 226 x 4
	1,42
	Glued


	2/3
	[image: ]
	Inner upper and lower cover - ASM
	Aramid fiber 9 layers
	955 x 757x 4
	3,37
	Glued

	4
	[image: ]
	Door lock cover
	High Strength Steel (HSS)
	344 x 210 x 2
	1,19
	Screwed

	5
	[image: ]
	Door front cover
	High Strength Steel (HSS)
	207 x 205 x 2
	1,19
	Glued

	6
	[image: A blue and green square

Description automatically generated]
	Moveable armored glass 
	Glass layers + Polymers
	720 x 520 x 18
	15,09
	Screwed

	7
	[image: A blue triangle object with a blue edge

Description automatically generated]
	Fixed armored glass
	Glass layers + Polymers
	190 x 400 x 18
	1,25
	Glued

	8
	[image: ]
	Lower rear cover 
	High Strength Steel (HSS)
	395 x 310 x 2
	1,46
	Glued

	9
	[image: ]
	Upper frame cover
	High Strength Steel (HSS)
	905 x 475 x 2
	1,22
	Glued

	10
	[image: ]
	Rear door lock cover
	High Strength Steel (HSS)
	63 x 210 x 2
	1,78
	Glued

	11
	[image: ]
	Inner front  panel cover
	High Strength Steel (HSS)
	127 x 572 x 2
	8,82
	Glued

	12
	[image: ]
	Fixed  glass channel cover
	High Strength Steel (HSS)
	  49 x 367 x 2
	2,57
	Glued
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