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Fig. S1 SEM images of MIL-68 (In) MOF (a) and In2S3-8h (b, c).
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Fig. S2 XRD pattern of In2S3-8h (a). The full XPS spectrum of In2S3/C (b).
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Fig. S3 The cycling performance of In2S3-8h at the current density of 0.5 A·g−1 (b). Rate performance of In2S3-8h at different current densities (b). The Nyquist plots of In2S3/C, In2S3-8h and commercial In2S3 (c). 
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