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Fig. S1 The FT-IR spectra of PAN nanofibers aerogel (a), supercritical dried (b) and ambient pressure dried (c) polyacrylonitrile nanofiber-reinforced silica aerogel
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Fig. S2 The TG curves of PAN nanofibers aerogel and APD-EPNR silica aerogel
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Fig. S3 The energy consumed as a function of cycle number of APD-EPNR silica aerogel
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