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 Due to the increase in the surface and size of polymer particles in the structure of the composite, the conductivity is slightly higher than that of the nanocomposite. Therefore, it can be concluded that in resistors that are used to limit a certain amount of electric current, the nanocomposite structure is preferable to the composite structure.
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