[bookmark: _Hlk141912357]Supplementary Figure 1. Flow cytometry gating strategy for SARS-CoV-2 Spike-protein specific PBMCs expression of CD4+IL-17 in stimulated (left) and unstimulated (right) samples of each MIS-C_A (Panel A), MIS-C_C (Panel B) and COVID-19 (Panel C). 
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Supplementary Figure 2. Flow cytometry gating strategy for SARS-CoV-2 Spike-protein specific PBMCs expression of CD8+IL-17 in stimulated (left) and unstimulated (right) samples of each MIS-C_A (Panel A), MIS-C_C (Panel B) and COVID-19 (Panel C). 
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Supplementary Figure 3. Flow cytometry gating strategy for SARS-CoV-2 Spike-protein specific PBMCs expression of CD8+IFN-γ in stimulated (left) and unstimulated (right) samples of each MIS-C_A (Panel A), MIS-C_C (Panel B) and COVID-19 (Panel C). 
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