eTable 1. Quality Assurance Metrics: Linewidth (LW) and signal-to-noise ratio (SNR) are presented for NAA; LW. and % Cramer Rao Lower Bounds (CRLB) are presented for GABA. Mean values, range and % CoV are shown as the well as the range of the median absolute deviation (MAD-range). This metric runs from the (median – 3x the median absolute deviation) to (median + 3x the median absolute deviation) and is considered a more reliable metric for outlier detection than mean +/- 3xSD
	
	NAA LW
	GABA LW
	NAA SNR
	NAA LW (Edit-off)
	GABA % CRLB

	Mean
	6.7
	24.0
	41.6
	6.4
	15.2%

	Range
	4.6-12.1
	18.0-30.0
	26.1-56.6
	4.7-13.2
	10.8%-19.5%

	CoV
	27%
	20%
	17%
	30%
	16.3%

	MAD-range
	4.2-8.1
	15.0-39.3
	29.5-55.3
	4.3-7.5
	10.2%-19.7%
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