Supplementary Material
Experimental model is printed on a Picaso 3D printer using ABS plastic. The printing area of the Picaso printer is 200×200×210 mm3, thus, the working model was build of 9 patches replicating the area of 700×700 m2. Fig. 1 shows an overall view of experimental model. The location of the extended source of impurity is indicated by a red frame, black color indicates the observation area.
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	Fig. 1 Overall view of experimental model: (a) - volumetric image; (b) - top view












The process of impurity propagation is shown in Fig. 2.
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	Fig. 2 Visualization of impurity distribution
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