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Fig. S2. SEM of Cu-Co-Ni-S/CP at different concentrations of CuCl2·2H2O solutions: (A) 0.5 mM; (B) 1 mM; (C) 2 mM; (D) 3 mM.
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Fig. S3. CVs of CP electrodes measured in the applied potential range from 0.00 V to +0.10 V at various scan rates. 
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Fig. S4. Effects of experimental conditions on the current density response of 0.1 mM glucose. (A) Applied potential; (B) NaOH concentration.
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Fig. S5. The reusability test of Cu-Co-Ni-S/C electrode.
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