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Procedure Steps

buld be paid to design features  Parameters (acc. to ISO 17665, EN 13060, EN 285

d holes, threads, undercuts  and AAMI TIR12) « Select the appropriate platform according to the
markings on the scan post.

« Clean the implant or analog platform area.

Method | Steam(EU™) | Steam Steam

bn products for visibility and
jon with the naked eye. Dynamic

oonens forproperassembly |9 | aremont | 20K | G it e o i 1‘3.?‘;%55":5(? erounded
Temperature | 134°C 132°C (270°F) | 135°C (275°F) side, facing lingual-
movable partsfor correot (TP +Tighten the sorew at 20Ncm.
Timet |3minves | 4mnvtes | 10mines + Scanusing an intra-oral o deskiop scanner according

omponents for completeness [T T T T o mines t0 scanner manufacture instructions. There is no

need for special pre-scanning treatment.

products. * Minimum exposure times, the operating times are longer and

may vary depending on the device. ** EU customers are required

o use these steam sterilzation parameters « Select the abutment level scan post according to
nts frequired, and place inakit the marking on the scan post.
Jouch which is legally marketed « The Multi-Unit scan post fits both straight and
DA-cleared) for use with the  The product must be stored ina dry placeiin the original angulated Multi-Unit abutments.
ation parameters. Packaging  packaging at room temperature and ot exposed 0.+ Glean the abutment or analog platiorm area.
bquirements accordingto DIN - direct sunlight. Incorrect storage may influence device

« Place the scan post on the abutment/analog with
LAMIST79and AAMITIRT2.  characteristics leading to failure. flat side to face buccal and the rounded side, to
age must have a sterilization face lingual
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