[bookmark: _GoBack]Table. 3: Thermodynamic parameters for safranin removal by various adsorption systems under study at 25 ֯C (sorbent dose: 2 g L¯¹; pH 7; initial safranin concentration: 120 mg L¯¹).


	Polymer sample                     T (K)                                 ∆G0 (kJ mol ⁻1)                 ∆H°( kJ mol ⁻1)             ∆S(kJ k⁻1 mol ⁻1)                            

	P(AA-co-MMA)                    298                                      -6.23                                    -61.15                               -0.18

	                                                    313                                      -1.13                                             

	                                                    323                                     -10.53

	CMC/p(AA-co-MMA)      298                                       -6.53                                     -48.24                               -0.11

	                                                    313                                      -4.94

	                                                    323                                      -7.70




