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Fig. S2 Colour and SV5 for 3 groups of sludge, from left to right, CAS, HPB(＜75μm），HPB(75-150μm）.
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Fig. S3 Microscopic results of sludge in 3 reactors after long-term CAS
HPB(＜75μm)
HPB(75-150μm)
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