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The crushed PKS sample is placed into heating mantle through quartz reactor. The HTL yield such as carbonaceous residue (char) can be obtained directly from quartz reactor. Bio-oil and Bio-gas yield can be separated by condenser from volatile matter for further characterizations.

