· Wall-climbing drilling robot designed for working in confined spaces
· The normal accuracy is ≤0.5°
· Normal positioning is achieved by synergy of mechanical expansion mechanism and joint torque control
