

Highlights

· This study presents a novel approach for hand motion detection using surface electromyography signals and a U-Net architecture along with metaheuristic optimization. 
· Bayesian optimization refines the BiLSTM model's architecture, boosting accuracy and reducing variance, thus improving overall performance. 
· The hybrid structure achieves 90.23% accuracy across six databases, signifying a significant enhancement compared to previous models.
