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[bookmark: _Hlk90054973]Fig. S1 Flow chart of preparation of 3D TiO2/Cu2O on Cu foam (a) and photocatalytic degradation experimental device (b).
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