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The dense structure of Fe-Zn alloy on the surface of Fe foam enhances the corrosion resistance of current collector, significantly boosting the discharge capacity and cycle stability of NaⅡZn liquid metal battery.
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