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Highlights
· Combining GEM and EIS allows in situ determination of the cement paste porosity.
· The pore solution conductivity of each cement paste is almost constant.
· The corrosion product diffusion does not significantly affect the porosity.
· The porosity results measured from EIS and MIP are in good agreement.
· The partly saturated pores lead to an underestimation of the total porosity.
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