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Table 1. Real meteorological climate data of the photovoltaic power plants center OUED-NECHOU, Ghardaïa.

	Studied days
	Ambient Temperature C°
	Humidity %

	January 1st, 2016
	20.70
	45.26

	May 1st, 2016
	29.38
	21.64

	July 1st, 2016
	36.31
	15.24

	October 1st, 2016
	30.2
	54.42



	Studied days
	Wind velocity (m/s)
	Sunshine (h)

	January 1st, 2016
	0.91
	11.13

	May 1st, 2016
	5.51
	15.46

	July 1st, 2016
	3.70
	15.26

	October 1st, 2016
	4.15
	13.04



[bookmark: _Hlk164434195]Table 2. The caption must be followed by the table.

	PV-Tech
	a-Si
	CdTe
	mc-Si
	pc-Si

	Type
	SCHOTT ASI 103
	FIRST SOLAR FS-380
	Atersa A-250M
	ATERS AA-235P

	Peak Power [Wp]
	103
	80
	250
	235

	Peak Power Tolerance [Wp]
	0 /+2,99
	±5
	0 /+5
	0 /+5

	Module Performance %
	7,1
	11,1
	15.35
	14,43

	Max Voltage (Vmpp) [V]
	30,4
	48,5
	30,35
	29,04

	Max Intensity (Impp) [A]
	3,39
	1,65
	8,24
	8,10

	Surface [m2]
	1,45
	0,72
	1,63
	1,63

	Open Circuit Voltage [V]
	41,1
	60,8
	37,62
	36,94

	Short Circuit Current [A]
	4,00
	1,88
	8,79
	8,64

	The System Max Voltage [V]
	1000
	1000
	1000
	1000

	NOCT [°C]
	49
	45
	47 ±2
	47 ±2

	Temperature Coefficient Isc [°K]
	+0,08 %
	+0,04%
	+0,03 %
	+0,04%

	Temperature Coefficient Voc [°K]
	-0,33 %
	-0,20 %
	-0,34 %
	-0,32 %

	Temperature Coefficient Pmax [°K]
	-0,20 %
	-0,27 %
	-0,43 %
	-0,43 %

	Wight [Kg]
	20,8
	12
	21,5
	21,5

	Dimensions [mm]
	1308 × 1108×35
	1200 × 600×6,8
	1645 × 990×40
	1645 × 990×40

	Cells
	72
	154
	60
	60



