Supplementary material:
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Fig.S1. Thin film thickness measurement using Profilometer
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Fig.S2. Image of the dark field photomask used for channel creation and light field photomask used for contact metallization.
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Fig.S3. Conventional XRD of ZnO thin film deposited at room temperature with different Ar:O2 flow rate
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