
HIGHLIGHTS

· Tukey’s test revealed that both rotation and type of tool impact the entry hole.
· Only the type of tool affected the exit hole;
· The tool angle influences the delamination;
· Diamond tool for entry/exit hole exhibited superior finishing;
· [bookmark: _GoBack]The 140° tool had less occurrences of entry delamination compared to the 118° tool.
