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[bookmark: _bookmark38]Figure S1. Tree-distributed homology nodes with number of tree layers and branches per layer. 
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Figure S2. Different pilot-tone power in the modulation signal impact on receiver optical power penalty.
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Figure S3. Detailed BER performance for the X- and Y-polarization of 4 tributaries dual-polarization 16-QAM signals.
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